PERFORMANCE:
							Feet	Meters		Remarks
Takeoff distance, over 50ft obstacle			1250			with zero wind. (Begin rotation at 60mph, +6 trim)
Takeoff run				
Short-field takeoff, over 50 ft obstacle		950			
Short-field takeoff run				
Landing distance, over 50ft obstacle			1370		
Landing run				
Short-field landing distance, over 50ft obstacle				
Short-field landing run					
Maximum Operating Altitude				17,500			FAA Operational Ceiling
Service ceiling	22,000		
							NM	SM	KM	
Range, maximum cruising power at 3000rpms		
Range, economy cruising power with 30 minutes 		950
reserve, 2600rpms at 22" MP.			
Range, maximum cruising power, max payload			
Range, economy cruising power, max payload				
							MPH	KTS	KM/HR	
Maneuvering 						142	123	229	True Indicated
Max. structural cruising (Max. Operating Speed) (Vmo)	200	174	322	True Indicated
Never Exceed (Vne)					270	235	435	True Indicated
Flaps extended - Half (20o) (Vfe)			150	130	241	True Indicated
Flaps extended - Full (40o)				125	109	201	True Indicated
Landing gear extended - revised VLO			180	156	290	True Indicated
Maximum level speed (TAS)				225			at Sea Level
Cruising speed (TAS) - 70% NRP				212			at 10,000ft / 3,048m
Economy cruising speed (TAS)				190			at 10,000ft / 3,048m
Takeoff speed						82	71	132	
Landing speed						87	
Best rate-of-climb speed (Vy)				110	
Best Angle of Climb speed (Vx)				10	10	10
Minimum Control speed (Vmc)				81	69	129
Stall Speed (Clean) (Vsi)				67	58	108	
Stall Speed - Full Flaps - power off			60	52	97	
Stall Speed - Full Flaps - power on			40	35	64	

							FPM	MPM		
Initial Rate of Climb					1,200	110
Initial Rate of Climb - Single-engine			200	100 estimated
Max. Rate of Climb at Sea Level				1,700	140		
Max. Rate of Climb at Sea Level, single engine 		400	122		
