PERFORMANCE:
							Feet	Meters		Remarks
Takeoff distance, over 50ft obstacle			1500			with zero wind. 
(Begin rotation at 80mph, +2 trim)

Takeoff run				
Short-field takeoff, over 50 ft obstacle		1200
		
Short-field takeoff run				
Landing distance, over 50ft obstacle			1605		
Landing run				
Short-field landing distance, over 50ft obstacle				
Short-field landing run					
Maximum Operating Altitude				17,500			FAA Operational Ceiling
Service ceiling	24,300		
							NM	SM	KM	
Range, maximum cruising power at 3200rpms		
Range, economy cruising power with 30 minutes 		1400
reserve, 2600rpms at 22" MP.			
Range, maximum cruising power, max payload			
Range, economy cruising power, max payload				

							MPH	knots	km/hr	
Maneuvering 						160	139	257	True Indicated
Max. structural cruising (Max. Operating Speed) (Vmo)	210	182	338	True Indicated
Never Exceed (Vne)					270	235	435	True Indicated
Flaps extended – Half (Vfe)				150	130	241	True Indicated
Flaps extended – Full					130	113	209	True Indicated
Landing gear extended 					180	156	290	True Indicated
Maximum level speed (TAS)				260	226	418	at 10,000’
Maximum cruising speed (TAS)				
Cruising speed (TAS) - 70% power			210	182	338	at 10,000ft / 3,048m
Takeoff speed						99	86	159	
Landing speed						92.5	80	149	
Best rate-of-climb speed (Vy)				120	104	193	
Best Angle of Climb speed (Vx)				
Minimum Control speed (Vmc)				
Stall Speed (Clean) (Vsi)				79	69	127	
Stall Speed (Dirty) (Vso)				71	62	114
	
							fpm	mpm		
Initial Rate of Climb				
Max. Rate of Climb at Sea Level				1,625	495		
Max. Rate of Climb at Sea Level, single engine 		310	94		
	
