"Battery Start"
CSD DISC Switches NORMAL
L & R Gen switches RESET/ON
AC/DC Bus X-tie Switches OPEN/OPEN
Fuel levers OFF
Fuel X-feed off
Cabin Alt Control ... AUTO/VALVE Open (not sure if this is modeled)
Pneumatic Crossfeed Levers OPEN (this was my big issue, these two levers on the bottom of the pedestal to the left and right of the rudder trim wheel, must open to provide APU bleed air to the engines for air starting ...)
Emergency-Power Switch ON (Again .. who'd have thought?)
Anti Collision light ON
Check Pneumatic pressure for sufficient bleed air pressure
START Pump switch ON
Right Engine START

Observe N2 to 15-20% Fuel on
Check Oil Pressure, EGT for temp rise, N1 for rotation

when stable ... START Switch off

Repeat for LEFT

when both stable:

EMERGENCY Power OFF
AC BUS X-TIE switch AUTO
FUEL PUMP Switches ... AS DESIRED
START PUMP ... OFF


Many Many congratulations to Samuli for this awesome panel ... I am running in FS9.

Hope this 