DEHAVILLAND DASH8-Q300
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 36,803 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed @ FL170 | 242 KIAS
VMO - Maximum Operating Speed @ FL200 | 232 KIAS
VMO - Maximum Operating Speed @ FL250 | 214 KIAS
MMO - Maximum Operating Speed Mach | .50 Mach
Turbulent Air Penetration Speed | 190 KIAS
VA - Maneuvering Speed | 177 KIAS
VMC - Minimum Control Speed | 103 KIAS
VX - Two-engine Best Angle-of-Climb | 135 KIAS
VY - Two-engine Best Rate of Climb | 145 KIAS
Best Glide Speed both engines inoperative | 135 KIAS

VFE - Maximum Flaps Extended Speed

Flaps | KIAS
Flaps 5 | 163
Flap 10 | 154
Flap 15 | 150
Flap 35 | 138

V1 - Takeoff Decision Speed dry runwayStandard temperature, 500 ft pressure altitude
Standard temperature, 500 ft pressure altitude

37,000 lbs | 142 KIAS
<28,000 lbs | 132 KIAS

VR - Rotation Speed dry runway - flaps 15
Standard temperature, 500 ft pressure altitude

37,000 lbs | 145 KIAS
<28,000 lbs | 135 KIAS

V2 - Takeoff Safety Speed dry runway - flaps 15
Standard temperature, 500 ft pressure altitude

37,000 lbs | 148 KIAS
<28,000 lbs | 142 KIAS

VREF - Landing Approach Speed - flaps 35 - gear down

37,000 lbs | 144 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.

Quick Reference - Panel Help

Quick Reference - VC Panel Help

Quick Reference - OVERHEAD

| Quick Reference - AP SPEED HOLD (BETA) |

| Quick Reference - GROUND HANDLING |
| Quick Reference - ALTITUDE SELECT |
| Quick Reference - THROTTLE QUAD |

+++NOTAMS+++
**** VERY IMPORTANT ****
Although the groundhandling5 gauge doesn't use FSUIPC itself
if you have the unregistered version of FSUIPC V4.0.0 or V4.0.1
(the very first FSX versions) installed
you MUST upgrade to V4.0.2 or higher
otherwise the Pushback-turn will not work.
If you haven't got a clue what FSUIPC is
then just ignore this remark.
**** IMPORTANT--IMPORTANT--IMPORTANT****
Due to differences in the Brakes implementation in FSX
with respect to the use of Toebrakes pedals,
activate (remove the "//" in front of the line)
gauge03= ONLY when you use proportional
toebrake pedals, like the CH Pro Pedals.
Removing the "//" will force the
Taxispeed gauge to use proportional Brake
commands (like your pedals)
instead of normal Brake commands.
Open the Panel_Docs folder for information on operating this aircraft.
Use Shift E to open the Pax Door.
Use Shift E+2 to open the Luggage Doort.
To Raise your seat higher in the VC - press SHIFT+ENTER.

Copyright 2007 - Premier Aircraft Design