BOMBARDIER LEARJET 60 PROCEDURES
For detailed instructions on how to fly this aircraft, see the Learjet 45 Aircraft Information articles in the Learning Center. For suggested speeds, see the Reference page of the Kneeboard. Note that most actions can also be performed using the mouse.

To... | Press...
Display/hide GPS | SHIFT+2
Display/hide throttle quadrant | SHIFT+3
Display/hide Ground Handling | SHIFT+4
Display/hide Timer/OAT | SHIFT+5
Display/hide Radio | SHIFT+6
Display/hide Fuel Qty/Flow | SHIFT+7
Display/hide Primary Flight Display | SHIFT+8
Display/hide Multi Function Display | SHIFT+9

BEFORE STARTING ENGINES
[ ] Gear | CHECK DOWN
[ ] BATT Switch | ON
[ ] L and R GEN Switches | OFF
[ ] Flight Controls | CHECK
[ ] Engine Instruments | CHECK
[ ] Fuel Quantity | CHECK
[ ] Fuel Crossfeed Button | CHECK ON
[ ] Fuel Crossfeed Light | CHECK EXTINGUISHED
[ ] De-ice | OFF
[ ] Aircraft Lighting | OFF
[ ] Parking Brake | SET (press CTRL + PERIOD key)
[ ] Trim | AS DESIRED (with Num Lock off press Num Pad 1 or Num Pad 7 as necessary)
[ ] Altimeters | SET
[ ] Standby Instruments | SET
[ ] Takeoff Data (V1, VR, V2) | COMPUTED and SPEEDS SET (see the Reference page of the Kneeboard)
[ ] Avionics Master Switch | ON
[ ] Avionics | SET FOR DEPARTURE
STARTING ENGINES |
Press CTRL+E to initiate engine autostart sequence, or:
[ ] Beacon/Strobe Switches | Set On
[ ] Parking Brake | SET (press CTRL + PERIOD key)
[ ] Thrust Levers | IDLE (press F2 or F3 as necessary)
[ ] Fuel Flow | ON (press CTRL+SHIFT+F4)
[ ] L Start Switch | ON (click and hold until engine starts)
[ ] L FF (Fuel Flow) | CHECK
[ ] L N1 increasing as L N2 increases | CHECK
[ ] L ITT | CHECK
[ ] L Oil Pressure | CHECK
[ ] L Engine Instruments | CHECK NORMAL
[ ] R Start Switch | ON (click and hold until engine starts)
[ ] R FF (Fuel Flow) | CHECK
[ ] R N1 increasing as L N2 increases | CHECK
[ ] R ITT | CHECK
[ ] R Oil Pressure | CHECK
[ ] R Engine Instruments | CHECK NORMAL
[ ] L and R GEN Switches | ON
BEFORE TAXI |
[ ] De-ice | AS REQUIRED
[ ] Spoiler Lever | Check (press SHIFT + / [FORWARD SLASH key])
[ ] Flaps | SET 8 OR 20 DEGREES (press F6 or F7 as necessary)
[ ] Flight Controls | CHECK
[ ] Aircraft Lighting | ON AS REQUIRED
[ ] Brakes | RELEASE (press PERIOD key)
TAXI AND BEFORE TAKEOFF
[ ] Brakes | CHECK (press PERIOD key)
[ ] Flight Instruments | CHECK
[ ] Engine Instruments | CHECK
[ ] Takeoff Data (V1, VR, V2) | CHECK (see the Reference page of the Kneeboard)
[ ] Nav Equipment | CHECK
[ ] Transponder | ON
[ ] Flaps | SET 8 OR 20 DEGREES (press F6 or F7 as necessary)
[ ] Trim | SET FOR TAKEOFF (with Num Lock off, press Num Pad 1 or Num Pad 7 as necessary)
[ ] De-ice | AS REQUIRED
RUNWAY LINEUP
[ ] Lights | ON
TAKEOFF |
[ ] Thrust Lever | T/O (press F3 until T/O)
[ ] Brakes | RELEASE (press PERIOD key)
[ ] VR | ROTATE
AFTER TAKEOFF |
[ ] Gear | UP AFTER POSITIVE RATE OF CLIMB
[ ] Flaps | UP AT V2+25
[ ] Yaw Damper | ON AS REQUIRED
[ ] Spoiler Lever | RET (press SHIFT + / (FORWARD SLASH key) until retracted)
[ ] De-ice | AS REQUIRED
[ ] L and R LDG-TAXI Light Switches | OFF
CLIMB |
CAUTION: Maximum thrust lever setting is MCR with full anti-ice on between 15,500 and 30,000 feet.
[ ] Altimeters | RESET TO 29.92 CROSSING 18,000 FEET
DESCENT |
[ ] De-ice | AS REQUIRED
CAUTION: Maximum thrust lever setting is MCR with full anti-ice on between 15,500 and 30,000 feet.
[ ] Altimeters | RESET TO LOCAL CROSSING 18,000 FEET
[ ] Fuel Quantities and Balance | CHECK
APPROACH |
[ ] Landing Data (VREF, VAPP) | COMPUTED and SPEEDS SET (see the Reference page of the Kneeboard)
[ ] Avionics and Radios | SET
[ ] Flaps | SET 8 OR 20 DEGREES (press F6 or F7 as necessary)
[ ] Spoiler Lever | ARM (press SHIFT + / [FORWARD SLASH key])
BEFORE LANDING |
[ ] Gear | DN (Check for 3 green lights) (press G)
[ ] L and R LDG-TAXI Light Switches | ON
[ ] Flaps | DN, check indication (press F7 until Dn)
LANDING |
[ ] Brakes | AS REQUIRED (press PERIOD key)
[ ] Spoilers | VERIFY EXTENDED
AFTER LANDING/CLEARING RUNWAY
[ ] Transponder | OFF
[ ] De-ice | AS REQUIRED
[ ] Lights | AS DESIRED
[ ] Spoiler Lever | RET (press SHIFT + / (FORWARD SLASH key) until retracted)
[ ] Flaps | b (press F6 until Up)
[ ] Thrust Lever | CUTOFF (press F2 until Cutoff)
SHUTDOWN |
[ ] Parking Brake | SET (press CTRL + PERIOD key)
[ ] De-Ice | OFF
[ ] Thrust Levers | IDLE (press F2 until Idle)
[ ] Fuel Flow | OFF (press CTRL+SHIFT+F1)
[ ] Lights | OFF
[ ] L and R GEN Switches | OFF
[ ] BATT Switch | OFF

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator.

Copyright © 2006 - Premier Aircraft Design