BOMBARDIER LEARJET 60
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 21,710 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 330 KIAS
MMO - Maximum Operating Speed Mach | .81 Mach
VA - Maneuvering Speed 13,850 lbs (sea level) | 150 KIAS
VA - Maneuvering Speed 13,850 lbs (20,000 ft) | 163 KIAS
VA - Maneuvering Speed 13,850 lbs (40,000 ft) | 195 KIAS
VA - Maneuvering Speed 23,500 lbs (sea level) | 198 KIAS
VA - Maneuvering Speed 23,500 lbs (20,000 ft) | 225 KIAS
VA - Maneuvering Speed 23,500 lbs (40,000 ft) | 245 KIAS
VLO - Maximum Gear Operating Speed | 200 KIAS
VLE - Maximum Landing Gear Extension Speed | 260 KIAS
Best Glide Speed (both engines inoperative) | 160 KIAS

Maximum Flap Placard Speeds

Flaps degrees | KIAS
8 | 250
20 | 200
40 | 150

V1 - Takeoff Decision Speed dry runway
Standard temperature, sea level pressure altitude

All conditions | 134 KIAS

VR - Rotation Speed dry runway
Standard temperature, sea level pressure altitude

All conditions | 135 KIAS

V2 - Minimum Climb Speed dry runway
Standard temperature, sea level pressure altitude

23,500 lbs | 160 KIAS

VREF - Landing Approach Speed flaps 40, gear down
Standard temperature, sea level pressure altitude

23,500 lbs | 140 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.

Quick Reference - Annunciator

Quick Reference - Ground Handling 4.0 for FS9

Quick Reference - GPWS3.3 Help

Quick Reference - NAV Help

Quick Reference - NAV Help

+++NOTAMS+++
Open the Panel_Docs folder for information on operating this aircraft.
Turn on Tool Tips
Panel Help available in the REF section of the Kneeboard
The Fuel Crossfeed Button must be in the On position for a balanced fuel burn.
Extinguish the Fuel Crossfeed annunciator light when lit by clicking on it with the mouse.
Use Shift E to operate the Passenger Airstair
Important... If using AUTOSTART (CTRL E)...
Check to make sure the Generators are switched to ON in the lower panel or VC
Use of Elevator trim is recommended in FSX
For Best Frame Rates...Keep Popup Windows Closed
Copyright © 2006 - Premier Aircraft Design