##
8-0 Fuel System Controls

1.
The engine fuel valves are on by default. It's recommented to leave them on. The valve for engine 2 is on the opposite side of the fuel panel.
2.
The APU fuel valve is off by default. You have to switch it on before you can start the APU.
3.
The fuel crossfeed switch is inop.
4.
The left and right outer wing tank fuel pump switches control the fuel feed to the engines for these tanks.
5.
Same as 4. just for the inner tanks.
6.
Same as 4. just for the center tank.
7.
Outer L anr R tank fuel display.
8.
Inner L anr R tank fuel display.
9.
Center tank fuel display.