##
9-1 ECAM AC Display

1.
The generator indication field displays the generator load, below the generator voltage and the AC frequency. When the generator is off, the GEN1 readout turns orange and the volts and freq. indication is replaced by a white OFF.
2.
Same as 1. for engine 2.
3.
The APU generator indication field is identical with the indication field of the engine generators.
4.
The TR1/2 indications turn orange when the AC 1/2 buses are unpowered.