##
1-1 FLIGHT CONTROLS Servo Controls

1.
The guarded servo push buttons control the servo control shut off valves for each hydraulic system. The clickspot to open the guard is located above the push button and the cursor changes to a hand with a minus (-) inside.
Normal:
No label is visible and the valve is open. All control surfaces are supplied with hydraulic pressure.
OFF(w):
The corresponding valve is closed and the pressure is removed from the control surfaces.