##
6-1 Engine Indications

1.
The reverser light is illuminated when the reverse nozzle is unlocked and the engine N1 is larger then 40%.
2.
The reverser unlocked light is illuminated when the reverse lever is pulled and the nozzle is unlocked.
3.
The N1 command pointer indicates the approximate N1 value for the current throttle position.
4.
The N1 needle indicates current N1 on a scale from 0 to 120 percent.
5.
The orange bug indicates the N1 limit computed by the TRC.
6.
N1 in percent with analog and digital indication.
7.
Exhaust gas temperature in degrees celsius with analog and digital indication.
8.
N2 in percent with analog and digital indication.
9.
Fuel flow in kilograms per hour with analog indication.
10.
Fuel used in kilograms with digital indication.
The counter is reset when the starter of the corresponding engine is activated.
11.
Oil pressure in PSI with analog indication.
12.
Oil quantity in PSI with analog indication.
13.
Oil temperature with analog and digital indication.
14.
Nacelle temperature in degrees celsius with analog indication.
15.
Fuel pressure in PSI with analog indication.
16.
N1 and N2 vibration with digital indication.