##
3-0 ND Rose Mode

1.
The yellow line indicates the current heading.
2.
The magenta triangle indicates the heading, which is set in the HDL SEL window on the glareshield.
3.
The compass rose goes from 0° to 360°.
4.
The green arrow indicates the VOR2 radial. The arrow is only visible when a VOR2 signal is received.
5.
The blue arrow indicates the ADF radial. The arrow is only visible when a ADF signal is received.
6.
The magenta arrow indicates the VOR1 radial. The arrow is only visible when a VOR1 signal is received and this signal is no ILS signal.
7.
The ground speed is always displayed in green numbers.
8.
The wind direction and the wind velocity are always displayed in green numbers.
9.
The display of the CDI and the OBS heading depends on the signal the NAV1 radio receives.
VOR signal:
The CDI is displayed in white and the OBS is displayed in green.
ILS signal:
The CDI is displayed in magenta and the OBS is displayed in green.
NO signal:
The CDI is displayed in white, whithout the deviation pointer and the OBS is displayed in green.
10.
The VOR1 station name is displayed in white and the VOR1 distance is displayed in green. When no VOR1 signal is received, the name readout is replaced by a dashed line.
When the NAV-GPS switch is in GPS position, the string VOR1 is replaced by a white GPS. The station name is also replaced by a white GPS and the GPS distance to the next waypoint is shown.
11.
The VOR2 station name is displayed in white and the VOR2 distance is displayed in green. When no VOR2 signal is received, the name readout is replaced by a dashed line.