P-166S Procedures

_____________________________________
PRE_FLIGHT CONTROL CHECK
Before flight verify you have full control
authority. Perform while sitting on the
ground with the engine off.
Elevator Up		16.9 
Elevator Down		10.4 
Aileron Up		25.0 
Aileron Down		15.0 
Rudder			21.6 

_____________________________________
TAKEOFF
Cowl Flaps		OPEN
Elevator Trim Set to		  05.4 deg
Rudder Trim Set to		  10.0 deg
Flaps			AS NEEDED
Throttle  100%
Brakes			RELEASE

_____________________________________
NORMAL CLIMB
Cowl Flaps		OPEN
Throttle  100%
Airspeed			 132 mph (IAS)

_____________________________________
CRUISE (BEST RANGE)
Throttle  80%

_____________________________________
COMBAT
Throttle  100%
Vy - Best Climb Speed	 110 mph (IAS)
Vno - Maneuvering Speed	 92 mph (IAS)
*** - Corner Speed		 121 mph (IAS)
Vne - Max Dive Speed	 410 mph
Max g			 3.3 g
		

_____________________________________
LANDING
Airspeed - Pattern		  83 mph (IAS)
Flaps			DOWN
Gear			DOWN
Airspeed - Over the Fence	  62 mph (IAS)
