BOEING B-52h
REFERENCE INFORMATION


Total aircraft weight with full fuel: 488,002 lbs

VMO - Maximum Operating Speed: 350 KIAS
MMO - Maximum Operating Speed: Mach .96 Mach
Turbulent Air Penetration Speed: 330 KIAS
VLO - Maximum Gear Operating Speed: 270 KIAS/.82 Mach
VLE - Maximum Landing Gear Extension Speed: 270 KIAS/.82 Mach

Maximum Flap Placard Speeds Flaps degrees   KIAS
      1   330
      5   310
      10   290
      20   280
      25   255
      30   230

V1 - Takeoff Decision Speed dry runway
Standard temperature, sea level pressure altitude
488,000 lbs (flaps 10) 160 KIAS
488,000 lbs (flaps 20) 155 KIAS

Standard temperature, 5,000' pressure altitude
488,000 lbs (flaps 10) 163 KIAS
488,000 lbs (flaps 20) 158 KIAS

VR - Rotation Speed dry runway
Standard temperature, sea level pressure altitude
488,000 lbs (flaps 10) 177 KIAS
488,000 lbs (flaps 20) 171 KIAS

Standard temperature, 5,000' pressure altitude
488,000 lbs (flaps 10) 179 KIAS
488,000 lbs (flaps 20) 173 KIAS

V2 - Minimum Climb Speed dry runway
Standard temperature, sea level pressure altitude
488,000 lbs (flaps 10) 188 KIAS
488,000 lbs (flaps 20) 181 KIAS

Standard temperature, 5,000' pressure altitude
488,000 lbs (flaps 10) 188 KIAS
488,000 lbs (flaps 20) 181 KIAS

VREF - Landing Approach Speed gear down
488,000 lbs (flaps 25) 188 KIAS
488,000 lbs (flaps 30) 181 KIAS
249,000 lbs (flaps 25) 134 KIAS
249,000 lbs (flaps 30) 129 KIAS
