BOEING B-52h PROCEDURES
 
To...Press...
Display/hide main panel SHIFT+1
Display/hide radios SHIFT+2
Display/hide GPS SHIFT+3
Display/hide throttle quadrant SHIFT+4
Display/hide overhead panel SHIFT+5
Display/hide clock SHIFT+6
Display/hide cockpit entrance SHIFT+E
Display/hide Bomb Bay Shift+E+2

PUSHBACK (if parked at a gate)

[ ] Pushback REQUEST (press SHIFT+P, then 1 for tail-left or 2 for tail-right, then press SHIFT+P to stop)
        
BEFORE START 
        
[ ] Parking Brake SET (press CTRL+PERIOD key)
        
ENGINE START 
        
Press CTRL+E to initiate engine autostart sequence.
        
AFTER START 
        
[ ] De-ice AS REQUIRED
[ ] Flight Controls CHECK
[ ] Autopilot SET AND OFF
[ ] Instruments CHECKED
[ ] Autobrake RTO (REJECTED TAKEOFF)
[ ] Avionics Switch ON
[ ] Avionics SET (press SHIFT+2 to display radio stack)
[ ] Trim SET
[ ] Beacon Light Switch ON
        
BEFORE TAKEOFF 
        
[ ] Flaps SET FOR TAKEOFF (press F7 as necessary)
[ ] Flight Director ON
[ ] Autothrottle ARM (if using TO/GA mode for takeoff)
        
TAKEOFF 
        
[ ] Brakes RELEASE (press PERIOD key)
[ ] Strobe Lights ON
[ ] Transponder ALT (press SHIFT+2 to display radio stack) 

[ ] Thrust Levers ADVANCE TO 1.05 EPR (press F2 or F3 as necessary)
[ ] Thrust Levers ADVANCE SMOOTHLY TO 100% N1 (press F2 or F3 as necessary)
      --or-- 
[ ] TO/GA Mode ENGAGE (press CTRL+SHIFT+R)
[ ] Thrust
 
VERIFY CORRECT FOR TAKEOFF

[ ] Airspeed 100 KIAS CALLOUT (100 KNOTS)
[ ] Airspeed V1 CALLOUT "V1" (140 KNOTS)
[ ] Airspeed VR CALLOUT "ROTATE" (165 KNOTS)
        
--ROTATE TO APPROX. 10 DEGREES PITCH UP--
        
[ ] Airspeed V2 CALLOUT "V2"
[ ] Landing Gear UP (WHEN POSITIVE CLIMB ESTABLISHED) (press G)
[ ] Autopilot Heading Select switch ON IF DESIRED
[ ] Airspeed MAINTAIN V2+15 KIAS (250-330 KNOTS)
[ ] Autopilot ENGAGE
[ ] Flaps START RETRACT ON SCHEDULE AT 1,000' AGL (press F6 as necessary)
        
CLIMB 
        
[ ] Autothrottle OFF
[ ] Landing Lights OFF ABOVE 10,000' MSL
[ ] Altimeter SET TO 29.92 CROSSING 18,000' MSL
        
CRUISE 
        
[ ] Thrust Levers AS DESIRED (press F2 or F3 as necessary)
[ ] Trim AS NECESSARY (press Num Pad 6 or Num Pad 7 as necessary)
        
DESCENT 
        
[ ] Airspeeds (VREF, VAPP) COMPUTED AND SET
[ ] Autobrake AS DESIRED
[ ] De-ice AS REQUIRED
[ ] Autopilot AS DESIRED
[ ] Thrust Levers AS DESIRED (press F2 or F3 as necessary)
[ ] Altimeter SET TO LOCAL SETTING CROSSING 18,000' MSL
[ ] Avionics SET (press SHIFT+2 to display radio stack)
[ ] Airspeed <250 KIAS BELOW 10,000' MSL
[ ] Landing Lights ON BELOW 10,000' MSL
[ ] Approach Procedure REVIEW
        
APPROACH 
        
[ ] Airspeed 180 Knots
[ ] Thrust Levers AS DESIRED (press F2 or F3 as necessary)
[ ] Flaps AS DESIRED (press F7 as necessary)
[ ] Autopilot AS DESIRED
        
LANDING 
        
[ ] Airspeed 160 Knots
[ ] Thrust Levers AS DESIRED (press F2 or F3 as necessary)
[ ] Landing Gear DOWN and CONFIRMED (press G)
[ ] Flaps AS DESIRED (press F7 as necessary)
[ ] Speedbrake

ARMED (press SHIFT + / [FORWARD SLASH key])

[ ] Autopilot AS DESIRED
[ ] Autothrottle ARM (if using TO/GA mode for go-around)
        
LANDING ROLL 
        
[ ] Thrust Levers CLOSED (press F2 or F3 as necessary)
[ ] Autothrottle CHECK OFF
[ ] Speedbrake Lever

CHECK FULL UP (press SHIFT+/ [FORWARD SLASH key] if necessary)

[ ] Thrust Levers REVERSE (press F2 until Reverse)
[ ] Thrust Levers IDLE AT 60 KIAS (press F3 until Idle)
[ ] AutobrakeOFF
[ ] Brake AS NECESSARY (press PERIOD key)
[ ] Autopilot CHECK DISENGAGED
        
TAXI-IN 
        
[ ] Speedbrake Lever DOWN (press / [FORWARD SLASH key])
[ ] Lights AS DESIRED
[ ] Flap Lever UP (press F6 until Up)
[ ] Transponder STBY
        
PARKING 
        
[ ] Parking Brake SET (press CTRL+PERIOD KEY)
[ ] Fuel Control Switches CUTOFF (press CTRL+SHIFT+F1)
[ ] De-ice OFF
[ ] Lights AS REQUIRED
[ ] Flight Director OFF

