Quick Notes to Fly the Spartan

1.  	Start engine
2.	Set flaps 15 if on short runway, otherwise optional
3.	Trim elevator to +3.5 and begin rollout
4.	Rotate at 90 MPH
5.	Retract gear and accelerate to 105+
6.	Retract flaps
7.	Trim for 1000fpm climb working your way down to +1.8 degrees trim
8.	Once desired altitude is reached, click ALT on the AP
9.	Reduce MP to 30" and RPM's to 2000 for cruise

To view/remove VC yoke, use the "/" key (Spoiler key)
To view/remove cigarettes, use shift+e, release and quickly press 2  (Cargo door key sequence)

If you do not have rudder pedals and wish to have a steerable tailwheel, change the aircraft.cfg Contact point 0 as noted there.  (Use Notepad to edit)

There is a "Cabin Light" switch on the VC panel for Daytime VC lighting to help in shadows.  Please do not use this at Dusk, Dawn, or Night flying as it destroys the backlighting of gauges.
