| Piaggio P-180 Avanti CheckList

| P-180 Pro cedures ______________________________________________________ PRE-FLIGHT CONTROL CHECK Before flight verify you have full control authority. Perform while sitting on the ground with the engines off. Elevator Up 15.0 Elevator Down 12.0 Aileron Up 23.0 Aileron Down 18.0 Rudder 20.0 ______________________________________________________ TAKEOFF Elevator Trim Set to 00.0 deg Rudder Trim Set to 00.0 deg Flaps 10.0 deg Throttle 100% Brakes RELEASE V1 90 KIAS V2 106 KIAS - ROTATE _______________________________________________________ NORMAL CLIMB Throttle 80% Airspeed 185 KIAS _______________________________________________________ CRUISE (FAST) Throttle 80% Airspeed 260 KIAS CRUISE (BEST RANGE) Throttle 60% Airspeed 210 KIAS _______________________________________________________ LANDING Airspeed - Pattern 120 KIAS Flaps DOWN Gear DOWN Airspeed - Over the Fence 100 KIAS _______________________________________________________ WARNING: ALL AEROBATIC MANOUVERS, INCLUDING SPINS, PROHIBED _______________________________________________________ IMPORTANT: PAYLOAD SETTING: PAYLOADS ARE SET BY DEFAULT NEAR MTOW, SO TAKEOFFS REQUIRE SOME CARE. LOWER THEM FOR EASIER HANDLING. IF YOU MOVE CG, REMEMBER TO SET TRIM ACCORDIGNLY. _______________________________________________________
|