SOCATA TBM 700
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information in the PILOT'S MANUAL. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 6 574 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 266 KIAS
Turbulent Air Penetration Speed | 170 KIAS
VLE - Maximum Gear Operating Speed | 178 KIAS
VLO - Maximum Gear Retraction Speed | 128 KIAS
VA - Maneuvering Speed | 184 KIAS
Optimum Glide Speed | 110 KIAS

Maximum Flap Placard Speeds

Flaps | KIAS
Approach | 178
Full extension | 122

VR - Rotation Speed dry runway, flaps up
Standard temperature, 5,000' pressure altitude

6 574 lbs | 85 KIAS

Cruise Climb

Sea level to 10,000 | 130 KIAS
10,000 to 15,000 | 130 KIAS
15,000 to 20,000 | 130 KIAS
20,000 to 25,000 | 130 KIAS
25,000 to 30,000 | 130 KIAS

VREF - Landing Approach Speed flaps down; gear down

6 250 lbs | 80 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.