DASSAULT FALCON 7X PROCEDURES
THIS CHECK LIST IS FOR USE ONLY WITH THE PAD FALCON 7X FLIGHT SIMULATOR MODEL
Note that most actions can also be performed using the mouse.

BEFORE STARTING ENGINES
[ ] Gear | CHECK DOWN
[ ] BATT Switch | ON
[ ] ALL 3 GEN Switches | OFF
[ ] Flight Controls | CHECK
[ ] Engine Instruments | CHECK
[ ] Fuel Quantity | CHECK
[ ] Fuel Crossfeed Button | CHECK ON
[ ] De-ice | OFF
[ ] Aircraft Lighting | OFF
[ ] Parking Brake | SET (press CTRL + PERIOD key)
[ ] Trim | AS DESIRED (with Num Lock off press Num Pad 1 or Num Pad 7 as necessary)
[ ] Altimeters | SET
[ ] Standby Instruments | SET
[ ] Avionics Master Switch | ON
[ ] Avionics | SET FOR DEPARTURE
STARTING ENGINES |
Press CTRL+E to initiate engine autostart sequence, or:
[ ] Beacon/Strobe Switches | Set On
[ ] Parking Brake | SET (press CTRL + PERIOD key)
[ ] Thrust Levers | IDLE (press F2 or F3 as necessary)
[ ] Fuel Flow | ON (press CTRL+SHIFT+F4)
[ ] L Start Switch | ON (click and hold until engine starts)
[ ] L FF (Fuel Flow) | CHECK
[ ] L N1 increasing as L N2 increases | CHECK
[ ] L ITT | CHECK
[ ] L Oil Pressure | CHECK
[ ] L Engine Instruments | CHECK NORMAL
[ ] R Start Switch | ON (click and hold until engine starts)
[ ] R FF (Fuel Flow) | CHECK
[ ] R N1 increasing as L N2 increases | CHECK
[ ] R ITT | CHECK
[ ] R Oil Pressure | CHECK
[ ] R Engine Instruments | CHECK NORMAL
[ ] L and R GEN Switches | ON
BEFORE TAXI |
[ ] De-ice | AS REQUIRED
[ ] Spoiler Lever | Check Retracted
[ ] Flight Controls | CHECK
[ ] Aircraft Lighting | ON AS REQUIRED
[ ] Brakes | RELEASE (press PERIOD key)
TAXI AND BEFORE TAKEOFF
[ ] Brakes | CHECK (press PERIOD key)
[ ] Flight Instruments | CHECK
[ ] Engine Instruments | CHECK
[ ] Takeoff Data (V1, VR, V2) | CHECK (see the Reference page of the Kneeboard)
[ ] Nav Equipment | CHECK
[ ] Transponder | ON
[ ] Flaps | SET 10 OR 20 DEGREES FOR TAKEOFF (press F6 or F7 as necessary)
[ ] Elevator Trim | SET FOR TAKEOFF ( +5 to +7º ) (with Num Lock off, press Num Pad 1 or Num Pad 7 as necessary)
[ ] De-ice | AS REQUIRED
RUNWAY LINEUP
[ ] Lights | ON
TAKEOFF |
[ ] Thrust Lever | T/O (press F3 until T/O)
[ ] Brakes | RELEASE (press PERIOD key)
[ ] VR | ROTATE
AFTER TAKEOFF |
[ ] Gear | UP AFTER POSITIVE RATE OF CLIMB
[ ] Flaps | UP AT V2+25
[ ] Yaw Damper | ON AS REQUIRED
[ ] Spoilers | CHECK RETRACTED
[ ] De-ice | AS REQUIRED
[ ] L and R LDG-TAXI Light Switches | OFF
CLIMB |
[ ] Altimeters | RESET TO 29.92 CROSSING 18,000 FEET
DESCENT |
[ ] De-ice | AS REQUIRED
[ ] Altimeters | RESET TO LOCAL CROSSING 18,000 FEET
[ ] Fuel Quantities and Balance | CHECK
APPROACH |
[ ] Landing Data (VREF, VAPP) | COMPUTED and SPEEDS SET (see the Reference page of the Kneeboard)
[ ] Avionics and Radios | SET
[ ] Flaps | SET 10 OR 20 DEGREES (as necessary)
[ ] Spoiler Lever | ARM (press SHIFT + / [FORWARD SLASH key])
BEFORE LANDING |
[ ] Gear | DN (Check for 3 green lights) (press G)
[ ] L and R LDG-TAXI Light Switches | ON
[ ] Flaps | DN, check indication (press F7 until Dn)
LANDING |
[ ] Brakes | AS REQUIRED (press PERIOD key)
[ ] Spoilers | VERIFY EXTENDED
AFTER LANDING/CLEARING RUNWAY
[ ] Transponder | OFF
[ ] De-ice | AS REQUIRED
[ ] Lights | AS DESIRED
[ ] Spoiler Lever | RET (press SHIFT + / (FORWARD SLASH key) until retracted)
[ ] Flaps | Retracted (press F6 until Up)
[ ] Thrust Lever | CUTOFF (press F2 until Cutoff)
SHUTDOWN |
[ ] Parking Brake | SET (press CTRL + PERIOD key)
[ ] De-Ice | OFF
[ ] Thrust Levers | IDLE (press F2 until Idle)
[ ] Fuel Flow | OFF (press CTRL+SHIFT+F1)
[ ] Lights | OFF
[ ] L and R GEN Switches | OFF
[ ] BATT Switch | OFF
NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator. Copyright © 2009 - Premier Aircraft Design