## HAWKER HURRICANE IId

# REFERENCE INFORMATION

For detailed instructions on how to fly this aircraft, please refer to the Hurricane IId .pdf document in the located in the Hurricane IId directory.

Total Flight Simulator aircraft weight with full fuel - 8218 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

# REFERENCE SPEEDS

Never Exceed Speed – 390 MPH IAS
Stall Speed Gear and Flaps up – 70-90 MPH IAS
Stall Speed Gear and Flaps down – 65-85 MPH IAS

Approach Speeds:

Engine assisted - 95 MPH IAS (105 MPH IAS flaps up).
Glide - 105 MPH IAS (115 MPH IAS flaps up).

Aerobatic Speeds:

Loop - at least 280 MPH IAS
Roll – 220-250 MPH IAS
Half Roll Off Loop – at least 300 MPH IAS
Upward Roll – 300 MPH IAS

Go-Around:

90 MPH IAS initially

Maximum Landing Gear Speed:

120 MPH IAS

Maximum Flap Speed:

120 MPH IAS

BEAM APPROACH:

NOTE: The airspeeds and power settings listed above MUST be increased for the IId to compensate for the extra parasite drag.

# AIRSPEED POSITION ERROR CORRECTION CHART

FUEL CONSUMPTION (APPROXIMATE)

ENGINE LIMITATIONS MERLIN XX (20)

Max. take-off to 1,000 ft - R.P.M....... 3,000

Max. take-off to 1,000 ft - Boost....... +12 lb/sq in.

Max. take-off to 1,000 ft - Temp, Coolant.. -----

Max. take-off to 1,000 ft - Temp, Oil... -----

Max. climbing, 1 hr. limit - R.P.M...... 2,850

Max. climbing, 1 hr. limit - Boost...... + 9 lb/sq in.

Max. climbing, 1 hr. limit - Temp, Coolant 125º C **

Max. climbing, 1 hr. limit - Temp, Oil.. 90º C

Max. weak continuous - R.P.M............ 2,650

Max. weak continuous - Boost............ + 4 lb/sq in.

Max. weak continuous - Temp, Coolant....... 105º C **

Max. weak continuous - Temp, Oil........ 90º C

Max. combat 5 mins limit - R.P.M........ 3,000

Max. combat 5 mins limit - Boost........ +14 lb/sq in.*

Max. combat 5 mins limit - Boost........ +16 lb/sq in.*

Max. combat 5 mins limit - Temp, Coolant... 135º C **

Max. combat 5 mins limit - Temp, Oil.... 105º C

NOTES :

* Combat boost is obtained by operating the boost control cut-out

** 115º C coolant temperature is permitted for short periods at cruising rpm.

Oil pressure - normal.................. 60-80 lb/sq in.

Oil pressure - minimum................. 45 lb/sq in.

Min. temp. for take-off - oil.......... 15º C

Min. temp. for take-off - coolant...... 60º C

Fuel pressure.......................... 8-12 lb/sq in.

----------------------------------------- END -----------------------------------------