BAe/McDONNELL-DOUGLAS HARRIER GR.Mk7 FLIGHT REFERENCE CARDS


Pre Start up Checklist
----------------------
Battery: On

RT: Pilot > ATC- ‘Ready for engine start, [your callsign]’
RT: ATC > Pilot- ‘[your callsign] clear engine start, call for clearance when ready for taxi’
RT: Pilot >ATC- ‘Starting engines, [your callsign]’


Start-up  Checklist
-------------------
Nav system: Align (activate fsnav)
Strobes: On
Canopy: Close
Nozzles: 0 degrees (fully aft)
H.P.cock(throttle): Ensure fully aft
Engine: Start
Check all indications
Control surfaces: Ensure full, free movement
Nozzles: Set 10 degrees
Landing gear lights: Ensure shows four greens
Nozzles/flaps: Check full, free movement 
AAR Probe: Check operation and seated correctly after check
Canopy: Open if req’d
Nozzles: minimum 10 degrees for taxi (Press F7 once from 0 deg)

RT: Pilot > ATC- ‘Engine start complete beginning preflight checks, [your callsign]’


Taxiing Checks
--------------
Brakes: Apply briefly
Nose wheel steering: Check operation

Pre Take Off Checks
-------------------
Canopy: Ensure closed and locked
Visor: Down
Strobes: As req’d
Landing lamp: On
Take-off brief: Complete

RT: Pilot > ATC- ‘[ATC Tower callsign], flight of one ready for departure, [your callsign]’
RT: ATC > Pilot- ‘[your callsign] cleared take off runway 12, winds 10 at 120’



Take-Off Checklist
------------------
Squawk Mode C 
Landing Lights ON 
Strobe ON 
RT: Pilot > ATC- ‘Cleared t/o [your callsign]’ 
Fuel: Check contents
Flaps/Nozzles: As req’d
Throttle: Idle to 55% (acceleration checks)

Perform Safe Take Off


After Take Off
--------------
Nozzles: Aft 0 degrees
Landing Gear: Up and lights out by 250kts
Warning lights: All out

RT: Pilot > ATC- ‘[ATC Tower callsign], airborne, [your callsign]’
RT: ATC > Pilot- ‘[your callsign] contact departure on 124.50’
RT: Pilot >ATC- ‘124.50 [your callsign]’


Landing checklist (following clearance)
---------------------------------------
Speed: Below 250kts
Airbrake: In,  warning light out
Landing gear: Down, 4 greens
Fuel: Contents Sufficient and balanced
Nozzles: As Req’d
Warning/caution lights: As req’d


After landing checklists
------------------------
Strobes: As req’d
Landing lamp: off
Nozzles: As req’d but no less than 10degrees

____________________________________


