INSTALLING THE GAUGES (for experienced users)

Unzip the archived gauges into your current MSFS path gauges folder.

ATTENTION
If you istall one of the GPS gauges like SL50, SL60, GX50, GX60 you *MUST*
install the Apollo ACU gauge too and vice versa. Otherwise for unknown reasons
on some computer configurations FS will not load the panel.

Add a line into your panel.cfg file where you want to install the gauge:

gaugeXX=gauge name!gauge name,  X-pos, Y-pos, W, H

where gauge name is the file name of the gauge without .gau;
X-pos, Y-pos - the X and Y position of the gauge in millimeters relative to the
panel background;
W and H - the width and the height of the gauge in millimeters.

Make sure that following system fonts are installed in the Windows Fonts folder:
- quartz.ttf
- glassga.ttf
These fonts come with the FS2002 Installation CD and are normally installed in
the \your FS path\Fonts directory. Copy them to \your Windows path\Fonts\
directory.

Unzip the archived font file
- glass.ttf
into \your Windows path\Fonts\ folder.

Unzip the archived sound files
- omi_test.wav
- soft_click.wav
into \your current MSFS path\Sound\ folder.

Gerd R. Nehr
GeRoN Brainware
gnehr@gat24.de