NORD AVIATION NORD 262 E FRÉGATE
REFERENCE INFORMATIONS
For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 23368 lbs 10.5 t

REMARQUE : To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 263 KIAS
MMO - Maximum Operating Speed Mach | Mach 0,58
Turbulent Air Penetration Speed | 170 KIAS
VLE - Maximum Gear Operating Speed | 184 KIAS
VLO - Maximum Gear Retraction Speed | 166 KIASs
VA - Maneuvering Speed | 184 KIAS
VMC - Minimum Control Speed | 94 KIAS
VX - Two-engine Best Angle-of-Climb | 125 KIAS
VY - Two-engine Best Rate of Climb | 140 KIAS
Best Glide Speed both engines inoperative | 135 KIAS

Maximum Flap Placard Speeds

Flaps | KIAS
Approach | 158
Full extension | 158

V1 - Takeoff Decision Speed dry runway; flaps up
Standard temperature, 5,000' pressure altitude

23368 lbs | 96 KIAS

VR - Rotation Speed dry runway, flaps up
Standard temperature, 5,000' pressure altitud

23368 livres | 102 KIAS

V2 - Takeoff Safety Speed dry runway, flaps up
Standard temperature, 5,000' pressure altitude

23368 lbs | 105 KIAS

Cruise Climb

Sea level to 10,000 | 170 KIAS
10 000 à 15 000 | 160 KIAS
15 000 À 20 000 | 150 KIAS
20 000 à 25 000 | 140 KIAS
25 000 À 30 000 | 130 KIAS
35 000 à 40 000 | 120 KIAS

VREF - Landing Approach Speed flaps down; gear down

22 000 lbs | 109 KIAS
21 000 lbs | 105 KIAS
20 000 lbs | 102 KIAS
19 000 lbs | 100 KIAS
18 000 lbs | 100 nœuds

NOTE : For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.

.

version 2

2004 july 14