NORD 262 E FRÉGATE PROCÉDURES

For detailed instructions on how to fly this aircraft, see the Reference page of the Kneeboard. Note that most actions can only be performed using the mouse

| Icons from left ti right
[ ] | Change viewa VFR /IFR
[ ] | Overhead panel
[ ] | Engines & Proplers panel
[ ] | Radios & Automatic Pilot
[ ] | GPS
[ ] | Kneeboard & référence
[ ] | Air Trafic Control
[ ] | Map

_______________________________________________________________

BEFORE ENGINE STARTING

[ ] | Make sure Parking Brakes are ON

_______________________________________________________________

ENGINE STARTING

[ 1 ] | Open Overhead panel Second icon from left
[ 2 ] | Put the batery awitch (1) ON (UP) The red lights of GENERATOR and CON1 will turn ON By clicking on the selector (4) verify the voltage on the voltmeter above the selector.
[ 3 ] | With the switch (2) put the converters ON to activate the panel gauges. The corresponding red lights will turn ON Do the same procedure for the CONV2 st right
[ 4 ] | Put the alternator swirch ALT (3) ON
| Close the overhead panel

[ 5 ] | Open the Engines & Proplers panel Third icon from the left
[ 6 ] | Open the engine start-up panel This panel is opened by clicking on the light bulbs found on the engines & proplers panel.
| The following steps are for the start-up of one engine. Repeat the steps for the second engine.
[ 7 ] | Open the red cap (5) and put the switch ON. Then close the red cap
[ 8 ] | Place the pump switchs (6) ON.
[ 9 ] | Put the selector (7) UP (Démarrage) The selector (7) has three positions. We can put the selector on the UP position by clicking above the selector
[10 ] | Increase slightly the throttle until the green light is ON.
[11 ] | Depress the start-up button (8) The red light turn ON Maintain action on the button until the red light turn OFF

_______________________________________________________________

TURBIB THE RADIOS ON

[ 1 ] | OuOpen the radio panel Fourth icon from the left
| The following steps describe the procedure for turning ON the radio and enter frewuencies of COMM1, NAV1, COMM2, NAV2 radois
[ 2 ] | Put the radio ON (COMM1, NAV1, COMM2, ou NAV2) by clicking on POWER
[ 3 ] | Enter the integer value of the desired frequency by clicking on the left button of each radio.
[ 4 ] | Enter the decimalr value of the desired frequency by clicking on the right button of each radio.
[ 5 ] | Put the ADF radio ON by clicking on the ADF position of the selector
[ 6 ] | The numbers of the ADF frequency can be changed by clicking below (+) or above (-) each bunberé

_______________________________________________________________

HORIZONTAL SITUATION INDICATOR (HSI)

[ 1 ] | Decrement by units The right & left knobs can be decremented by one degree by clicking with the mouse left button
[ 2 ] | Decrement by tens The right & left knobs can be decremented by ten degree by clicking with the mouse right button.

BEFORE TAKEOFF (RUNUP) |
[ ] Avionics | CHECK
[ ] Autopilot | CHECK
[ ] Electronic Pitch Trim Control | CHECK
[ ] Trim Tabs | SET (with Num Lock off press Num Pad 1 or Num Pad 7 as necessary)
[ ] Primary Governors | EXERCISE AT 1500 RPM
[ ] Autofeather | ARM
[ ] Manual Propeller Feathering | CHECK
[ ] Anti-ice | AS REQUIRED
[ ] Fuel Quantity, Flight, and Engine Instruments | CHECK
BEFORE TAKEOFF (FINAL ITEMS)
[ ] Annunciator Lights | EXTINGUISHED OR CONSIDERED
[ ] Transponder | ON ALT
[ ] Lights | AS REQUIRED
[ ] Anti-ice | AS REQUIRED
[ ] Takeoff speeds (V1, VR, and V2) | CONFIRM
TAKEOFF |
[ ] Brakes | HOLD
[ ] Power Levers | 100% N1 TURBINE RPM (OBSERVE ITT LIMITS) (press F3 as necessary)
[ ] Brakes | RELEASE (press PERIOD key)
[ ] VR | ROTATE TO APPROX. 10 DEGREES PITCH UP
[ ] Landing Gear | UP (WHEN POSITIVE CLIMB ESTABLISHED) (press G)
[ ] Airspeed | MAINTAIN V2 UNTIL CLEAR OF OBSTACLES
[ ] Flaps | UP (BLUE LINE, 125 KIAS MINIMUM)
CLIMB |
[ ] Climb Power | 90% N1 TURBINE RPM (OR AS DESIRED) (press F2 or F3 as necessary)
[ ] Propellers | 1600 RPM (OR AS DESIRED) (press CTRL+F2 or CTRL+F3 as necessary)
[ ] Propeller Synchrophaser | ON
[ ] Engine Instruments | MONITOR
[ ] Lights | AS REQUIRED
CRUISE |
[ ] Cruise Power | AS DESIRED (press F2 or F3 as necessary)
[ ] Engine Instruments | MONITOR
[ ] Autofeather | OFF
DESCENT |
[ ] Altimeter | SET
[ ] Autofeather | ARM
[ ] Fuel Balance | CHECK
[ ] Power | AS REQUIRED (press F2 or F3 as necessary)
BEFORE LANDING |
[ ] Autofeather | VERIFY ARMED
[ ] VREF | CONFIRM
[ ] Altimeter | SET
[ ] Flaps | APPROACH (press F7 until APPR)
[ ] Landing Gear | DOWN (press G)
[ ] Lights | AS REQUIRED
[ ] Anti-ice | AS REQUIRED
NORMAL LANDING --When landing is assured--
[ ] Flaps | DOWN (press F7 until DN)
[ ] Airspeed | VREF
[ ] Condition Levers | HIGH IDLE (press CTRL+SHIFT+F3 until fully in)
[ ] Propeller Levers | FULL FORWARD (press CTRL+F3 until fully in)
[ ] Power Levers | IDLE (press F2 until Idle)
--After touchdown-- |
[ ] Power Levers | GROUND FINE (press F2 until fully out)
[ ] Brakes | AS REQUIRED (press PERIOD key)
AFTER LANDING |
[ ] Engine Auto-Ignition | OFF
[ ] Anti-ice | OFF
[ ] Lights | AS REQUIRED
[ ] Transponder | STANDBY (press SHIFT+2 to display radio stack)
[ ] Trim Tabs | SET (with Num Lock off press Num Pad 1 or Num Pad 7 as necessary)
[ ] Flaps | UP (press F6 until UP)
SHUTDOWN AND SECURING |
[ ] Parking Brake | SET (press SHIFT+PERIOD key)
[ ] Avionics Master | OFF
[ ] Autofeather | OFF
[ ] Lights | OFF
[ ] ITT | STABILIZED AT MINIMUM TEMPERATURE FOR 1 MINUTE
[ ] Condition Levers | FUEL CUTOFF (press CTRL+SHIFT+F2 until fully out)
[ ] Propellers | FEATHER (press CTRL+F2 until fully out)
[ ] Battery and Generator Switches | OFF (below 15% N1)

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator.

version 2

2004 july 14