Crosswind correction and ground-speed calculator gauge for MSFS2004

2010© Freeware, Alexander Belov <a_belov@mail.ru>

Crosswind correction and ground speed calculator is a simple and easy-to-use instrument, usable for any aircraft developing airspeed from 200 to 500 kph (125 – 312 mph). It allows to calculate crosswind correction and ground speed using known values of aircraft speed and desired track angle, and wind velocity and wind direction.

Installation:

- Copy Vetrochet.cab to the GAUGES folder of your MSFS2004 installation.

- Open panel.cfg and insert in the windows declaration section following line:

WindowXX=Vetrochet

where XX is the number of new window.

Also insert a description for the new window as follows:


[WindowXX]
Background_color=0,0,0 
size_mm=1024,768
window_size_ratio=1.000  
position=0
visible=0
ident=30
window_size= 1.000, 1.000
window_pos= 0.000, 0.000

gauge00=Vetrochet!Vetrochet,  411,11,600,523


Read Vetrochet_R.pdf for more information.