Bombardier CRJ700-ER
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 71,727 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 330 KIAS
MMO - Maximum Operating Speed Mach | .85 Mach
Turbulent Air Penetration Speed | 280 KIAS/.73 Mach
VLO - Maximum Gear Operating Speed | 235 KIAS
VLE - Maximum Landing Gear Extension Speed | 270 KIAS/.80 Mach

Maximum Flap Place Card Speeds

8 | 225 KIAS
20 | 215 KIAS
30 | 185 KIAS
45 | 170 KIAS

V1 - Takeoff Decision Speed DRY RUNWAY, FLAPS 20
Standard temperature, sea level pressure altitude

72,000 lbs | 134 KIAS

Standard temperature, 5,000' pressure altitude

72,000 lbs | 138 KIAS

VR - Rotation Speed DRY RUNWAY, FLAPS 20
Standard temperature, sea level pressure altitude

72,000 lbs | 134 KIAS

Standard temperature, 5,000' pressure altitude

72,000 lbs | 138 KIAS

V2 - Takeoff Safety Speed DRY RUNWAY, FLAPS 20
Standard temperature, sea level pressure altitude

72,000 lbs | 146 KIAS

Standard temperature, 5,000' pressure altitude

72,000 lbs | 148 KIAS

VREF - Landing Approach Speed FLAPS 30, GEAR DOWN

72,000 lbs | 148 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.

    Quick Reference - EYEPOINT KEY COMMANDS

    Move Eyepoint Back

    CTRL+ENTER

    Move Eyepoint Down

    SHIFT+BACKSPACE

    Move Eyepoint Forward

    CTRL+BACKSPACE

    Move Eyepoint Left

    CTRL+SHIFT+BACKSPACE

    Move Eyepoint Right

    CTRL+SHIFT+ENTER

    Move Eyepoint Up

    SHIFT+ENTER

    Reset Eyepoint

    SPACE

Copyright 2004 - Premier Aircraft Design