Specifications Saab 340B

General characteristics

* Crew: 2 pilots, 1 flight attendant

* Capacity: 30, 33, 34 or 36 passengers

* Length: 19.73 m (64 ft 9 in)

* Wingspan: 21.44 m (70 ft 4 in)

* Height: 6.97 m (22 ft 11 in)

* Wing area: 41.8 m² (450 sq ft)

* Airfoil: NASA MS(1)-0316 / -0312 (root/tip)

* Empty weight: 8140 kg (17,945 lb)

* Loaded weight: 13,155 kg (29,002 lb)

* Powerplant: 2× General Electric CT7-9B turboprops, 1295 kW (1,735 shp) each

* Propellers: Dowty Rotol or Hamilton Standard 14RF19 four-blade constant speed propeller, 1 per engine

o Propeller diameter: 3.35 m (11 ft)

Performance

* Maximum speed: 523 km/h (282 kt IAS)

* Cruise speed: 467 km/h (252 kt IAS)

* Normal service range: 400-500 nm (34 passengers + baggage)

* Extended Range: 1730 km (935 nm)

* Cruise altitude 22,000 ft

* Service ceiling: 25,000 ft (commercial) / 31,000 ft (executive configuration) (7,600 m / 9,400 m)