EMBRAER 120ER BRASILIA BY PREMIER AIRCRAFT DESIGN
For suggested speeds, see the Referencepage of the Kneeboard.
Note that most actions can also be performed using the mouse.

For Microsoft Flight Simulator FS2004 & FSX

To... | Press...
Display/hide GPS | SHIFT+2
Magnify Annunciator Panel | SHIFT+3
Display/hide engine controls | SHIFT+4
Display/hide pushback/ground handling panel | SHIFT+5
Display/hide radio panel | SHIFT+6
Magnify Nav Panel | SHIFT+7
Magnify Engine Gauges | SHIFT+8

BEFORE ENGINE STARTING |
[ ] Parking Brake | SET (press CTRL+PERIOD key)
[ ] Landing Gear Control | CHECK "DOWN"
[ ] Power Levers | IDLE (press F2 until Idle)
[ ] Propeller Controls | (Automatic on this model)
[ ] Condition Levers | FUEL CUTOFF (press CTRL+SHIFT+F2 until fully out)
[ ] Fuel Quantity | CHECK
[ ] Anti-ice | ON (if required)
[ ] Beacon | ON
[ ] "Anti-ice" Annunciators | CHECK (press SHIFT+3 to magnify annunciator panel)
ENGINE STARTING (BATTERY) |
Press AUTO START BUTTON to initiate engine autostart sequence, or follow this sequence:
[ ] Battery Switch | ON
[ ] Beacon | ON
[ ] Propeller Area | CLEAR
[ ] Fuel Flow | ON (press CTRL+SHIFT+F4)
[ ] Engine Start Button | ON (click and hold until engine starts)
[ ] Condition Levers | LOW IDLE (after the N1 Turbine RPM has stabilized, 12% minimum)
[ ] ITT and N1 Turbine RPM | MONITOR
[ ] "FUEL PRESS LO" Annunciator | EXTINGUISHED
[ ] "OIL PRESS LO" Annunciator | EXTINGUISHED
[ ] Oil Pressure | CHECK
[ ] Condition Levers | HIGH IDLE
[ ] Both Generators | ON
[ ] Avionics Master Switch | ON
BEFORE TAKEOFF (RUNUP) |
[ ] Avionics | CHECK
[ ] Autopilot | CHECK
[ ] Pitch Trim Control | CHECK
[ ] Trim Tabs | SET (with Num Lock off press Num Pad 1 or Num Pad 7 as necessary)
[ ] Anti-ice | AS REQUIRED
[ ] Fuel Quantity, Flight, and Engine Instruments | CHECK
BEFORE TAKEOFF (FINAL ITEMS)
[ ] Annunciator Lights | EXTINGUISHED OR CONSIDERED
[ ] Lights | AS REQUIRED
[ ] Anti-ice | AS REQUIRED
[ ] Takeoff speeds (V1, VR, and V2) | CONFIRM
TAKEOFF |
[ ] Brakes | HOLD
[ ] Power Levers | 100% N1 TURBINE RPM (OBSERVE ITT LIMITS) (press F3 as necessary)
[ ] Brakes | RELEASE (press PERIOD key)
[ ] VR | ROTATE TO APPROX. 10 DEGREES PITCH UP
[ ] Landing Gear | UP (WHEN POSITIVE CLIMB ESTABLISHED) (press G)
[ ] Airspeed | MAINTAIN V2 UNTIL CLEAR OF OBSTACLES
[ ] Flaps | UP (200kts flap limit)
CLIMB |
[ ] Climb Power | 90% N1 TURBINE RPM (OR AS DESIRED) (press F2 or F3 as necessary)
[ ] Propellers | (Automatic on this model)
[ ] Engine Instruments | MONITOR
[ ] Lights | AS REQUIRED
CRUISE |
[ ] Cruise Power | AS DESIRED (Set Autopilot as required)
[ ] Engine Instruments | MONITOR
DESCENT |
[ ] Altimeter | SET
[ ] Fuel Quantity | CHECK
[ ] Power | AS REQUIRED (press F2 or F3 as necessary)
BEFORE LANDING |
[ ] VREF | CONFIRM
[ ] Altimeter | SET
[ ] Flaps | APPROACH (press F7 until APPR)
[ ] Landing Gear | DOWN (press G)
[ ] Lights | AS REQUIRED
[ ] Anti-ice | AS REQUIRED
NORMAL LANDING --When landing is assured--
[ ] Flaps | DOWN - (CHECK-Autopilot off for manual landing) (press F7 until DN)
[ ] Airspeed | VREF
[ ] Condition Levers | HIGH IDLE (press CTRL+SHIFT+F4
[ ] Propeller Levers | (Automatic on this model)
[ ] Power Levers | IDLE (press F3 until Idle)
--After touchdown-- |
[ ] Power Levers | IDLE or REVERSE THRUST (F2)
[ ] Brakes | AS REQUIRED (press PERIOD key)
AFTER LANDING |
[ ] Anti-ice | OFF
[ ] Lights | AS REQUIRED
[ ] Transponder | STANDBY
[ ] Flaps | UP (press F6 until UP)
SHUTDOWN AND SECURING |
[ ] Parking Brake | SET (press SHIFT+PERIOD key)
[ ] Avionics Master | OFF
[ ] Lights | OFF
[ ] ITT | STABILIZED AT MINIMUM TEMPERATURE FOR 1 MINUTE
[ ] Condition Levers | FUEL CUTOFF (press CTRL+SHIFT+F2 until fully out)
[ ] Propellers | Will feather automatically when engine shuts down
[ ] Battery and Generator Switches | OFF (below 15% N1)

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator FS2004 & FSX.