STANDARD OPERATING PROCEDURES

SHORTS SD3-60

WEIGHT LIMITATIONS

Maximum Ramp 26,553

Maximum Take-off 26,453

Maximum Landing 26,100

Designed Payload 7,500

Minimum Flight 15,800

SPEED LIMITATIONS

Max. Operating Vmo 196 kts

Maneuvering Va AUW 16,000 lbs. 129 kts

AUW 26,453 lbs. 160 kts

Flap Speed Vfe 5° 150 kts

15° 145 kts

30° 135 kts

Landing Gear Vlo 150 kts

Vle 162 kts

Min. Control Vmc Flaps 50° 83 kts

Vmc Flaps 15° 82 kts

OPERATING LIMITATIONS

Ambient Air Temperature -40 to +50 degrees

Airport Elevations Take-off & Landing, up to 8000 ft

Max. Certificated Altitude 20,000 ft

Load Factor Flaps up 1 to +2.8g

Flaps down 0 to +2.0g

DIMENSIONS

Span 74 ft 9.5 in

Length 70 ft 9.6 in

Height 23 ft 8.0 in

TIRE PRESSURES On Load

Main Wheels 112 psi +6/?0