Library description file for: ron_ez_highwayz.bgl
Automatically created by EZ-Scenery Manager

# Format for description files:
# GUID name
# GUID must consist of 32 hex digits. The format is identical to the one used in
# BGLCOMP (FS2004 SDK)

21F0D87F38AA4306BFCB3BC7F20B0431 2 Lane 2 degree ANGLE
21F0D87F38AA4306BFCB3BC7F20B0432 2 Lane ALL PASS long
21F0D87F38AA4306BFCB3BC7F20B0433 2 Lane ALL PASS medium
21F0D87F38AA4306BFCB3BC7F20B0434 2 Lane CURVE
21F0D87F38AA4306BFCB3BC7F20B0435 2 Lane NO PASS long
21F0D87F38AA4306BFCB3BC7F20B0436 2 Lane NO PASS medium
21F0D87F38AA4306BFCB3BC7F20B0437 2 Lane ONE PASS long
21F0D87F38AA4306BFCB3BC7F20B0438 2 Lane ONE PASS medium
21F0D87F38AA4306BFCB3BC7F20B0439 2 lane Red light
21F0D87F38AA4306BFCB3BC7F20B043A 4 Lane CURVE
21F0D87F38AA4306BFCB3BC7F20B043B 4 Lane LONG
21F0D87F38AA4306BFCB3BC7F20B043C 4 Lane Medium
21F0D87F38AA4306BFCB3BC7F20B043D 4 lane Red lights
21F0D87F38AA4306BFCB3BC7F20B043E innerstate CURVE
21F0D87F38AA4306BFCB3BC7F20B043F innerstate LONG
21F0D87F38AA4306BFCB3BC7F20B0440 innerstate Medium
21F0D87F38AA4306BFCB3BC7F20B0441 4 lane_2 lane Red lights
21F0D87F38AA4306BFCB3BC7F20B0442 4 lane_2 lane to 4 lane Red lights
