SAFETY & POWER ON
MAINTENANCE STATUS |  | CHECKED
DC METER SELECTOR |  | BAT
BATTERY SWITCH |  | ON
ELECTRIC HYDRAULIC PUMPS |  | OFF
APU BLEED SWITCH |  | OFF
LANDING GEAR LEVER |  | DOWN
FLAP LEVER |  | SET
RADAR |  | OFF
FIRE CONTROL PANEL |  | CHKD
APU | STAR & ON | BUSES

ORIGINATING/RECEIVING
ORIGINATING AND ALL EXTENDED OVERWATER FLIGHTS: CHECK ALL ITEMS. RECEIVING FLIGHTS: CHECK ALL ITEMS EXCEPT THOSE WICH ARE INTENDED
PREFLIGHT INSPECTIONS | VERIFY | COMPLETE
LOGBOOK, FORMS, | VERIFY | CHECKED
QRH | VERIFY | INSTALLED
GEAR PINS | (C) | STOWED
CIRCUIT BREAKERS | VERIFY | CHKD
O2 & INTERPHONE | VERIFY | CHKD
AFT OVERHEAD PANEL | (FO) | CHKD
LIGHT TEST | (C) | TESTED
FLIGHT CONTROL PANEL | (C) | CHKD
FUEL PANEL | (C) | CHKD
ELECTRICAL PANEL | (C) | CHKD
EQUIP COOLING | (C) | NORMAL
EMER EXIT LIGHTS | (C) | ARMED
SEATBELT/NO SMOKING | (C) | OFF/ON
ICE PROTECTION | (C) | CHKD
HYDRAULICS | (C) | CHKD
COCKPIT VOICE REC | (C) | TESTED
CARGO FIRE CONTROL PANEL | (FO) | CHKD
AIR COND & PRESS | (FO) | CHKD
WINDSHEAR WARNING | (C) | CHKD
FLT INSTS/RADIO ALTM | VERIFY | CHKD
ANTI-SKID | (C) | ON
PDCS/GPS | (C) | CHKD
RADAR | (C) | TCAS
GPWS | (C) | TESTED
FLAP LEVER | (C) | SET
STAB TRIM CUTOUT SWS | (C) | NORMAL
FIRE CONTROL PANEL | (C) | CHKD
TRANSPONDER | (C) | STBY
RUDDER & AIL TRIM | (C) | CHKD&ZERO
STATIC SELECTORS | VERIFY | NORMAL
ORIG/RECEIVING CKLST | (FO) | COMPLETE

BEFORE START
| FUELQTY | VERIFY | ___REQ,___OB
| OIL/HYD QTYS | (C) | CHKD/CHKD
(D) | FUEL PANEL | (C) | ___ PUMPS ON
| SEAT BELT SIGNS | (C) | ON
| WINDOW HEAT | (C) | ON
| HYDRAULICS | (C) | A^sOFF, B^SON
| PRESSURIZATION | VERIFY | SET
| ALTIMETERS/FLT INST | VERIFY | ___,___CHKD
| ENGINE INSTRUMENTS | (C) | SET
| AUTOBRAKE | (C) | RTO
| PDCS/GPS | (C) | SET
| SPEEDBRAKE | (C) | DOWN DETENT
(D) | PARKING BRAKE | (C) | SET
| RADIOS | VERIFY | SET
| DEPARTURE REVIEW | (C) | COMPLETE
| Ø
(D) | L&R PACKS&PRESS | (FO) | OFF,___PSI
| ANTI-COLLISION LIGHTS | (FO) | ON
| DOOR LIGHTS&LOCK | (FO) | CHKD
| BEFORE START CKLST | (FO) | COMPLETE

AFTER START
(D) | ELECTRICAL PANEL | (C) | GENERATORS ON
| HYDRAULICS | (C) | PUMPS ON
(D) | ENGINE ANTI-ICE | (C) | ON OR OFF
| PITOT HEAT | (C) | ON
(D) | AIR COND&PRESS | (FO) | ON, ON, FLT
| or SET for ___
| SHOULDER HARNESS | VERIFY | ON
| AFTER START CKLST | (FO) | COMPLETE

BEFORE TAKEOFF
RECALL | (C) | CHKD
FLT CTRLS/YAW DAMPER | VERIFY | CHKD
TAKEOFF DATA | VERIFY | CHKD &SET
FLAPS | VERIFY | ___GREEN LT
| DETENT
STAB & TRIM | VERIFY | ___ZERO,ZERO
T.O. BRIEFING | (C) | COMPLETE
Ø
T.O.MIN FUEL QTY | VERIFY | ___REQ,___OB
FLIGHT ATTERNDENTS | (FO) | NOTIFIED
STAR SWITCHES | (FO) | L IGN
TRANSPONDER | (FO) | TA/RA
BEFORE T.O. CKLST | (FO) | COMPLETE

AFTER TAKEOFF
FLAPS |  | UP NO LTS, DETENT
GEAR/AUTOBRAKE |  | UP/OFF
AIR COND & PRESS |  | CHKD & SET
START SWITCHES |  | OFF or L IGN
APU | OFF or ON |
AFTER T.O. CKLST | (PNF) | COMPLETE

PRELIMINARY LANDING
ALTIMETERS/FLT INST | VERIFY | ___,___CHKD
LANDING DATA | VERIFY | CHKD & SET
SHOULDER HARNESS | VERIFY | ON
AUTOBRAKE | (C) | ___SET or OFF
APPROACH BRIEFING | (C) | COMPLETE
PRELIM LDG CKLST | (PNF) | COMPLETE

LANDING
START SWITCHES | (PNF) | L IGN
RECALL | (PNF) | CHKD
SPEEDBRAKE | (PNF) | ARMED,GREENLT
GEAR | VERIFY | DOWN,3 GREEN
Ø
FLAPS | VERIFY | ___GREENLT
LANDING CKLST | (PNF) | COMPLETE

AFTER LANDING
TRANSPONDER | STBY
FLAPS | UP
STAB TRIM | SET
SPEEDBRAKE | DOWN DETENT
RADAR | STBY or TCAS
APU (If required) | START
START SWITCHES | OFF
FLT/GRD SWITCH | GRD
PITOT HEAT | OFF
WINDOW HEAT | OFF or ON
APU GEN SWITCHES | ON or OFF
AFTER LDG CKLST | COMPLETE

PARKING & SECURING
PARKING BRAKE | (C) | SET or OFF
START LEVERS | (C) | CUTOFF
FUEL PANEL | (C) | SET
ELEC HYD PUMPS | (C) | OFF or ON
ICE PROTECTION | (C) | OFF
SEAT BELT SIGN | (C) | OFF
ANTI-COLLISION LIGHT | (FO) | OFF
AIR COND | (FO) | SET
QRH | VERIFY | POSITIONED
PARKING CKLST | (FO) | COMPLETE
THE FOLLOWING ITEMS COMPLETED ONLY AT TERMINATION
GALLEY POWER | OFF
EMER EXIT LIGHTS | OFF
L & R PACKS | OFF
RADAR | OFF
APU/GROUND POWER | ON or OFF
BATTERY SWITCH | ON or OFF
SECURING CKLST | COMPLETE
(D) Denotes item for delayed engine start checklist