    PREMIER AIRCRAFT DESIGN

    DORNIER Do328JET model for FS2004 and FSX
    REFERENCE INFORMATION

    NOTES:

    (1) To adjust fuel load and and passenger/freight load, in the FS9/FSX Aircraft menu click 'Fuel & Load'
    (2) To show and hide yoke in the VC use keys Shift-W (FS9) Ctrl-W (FSX)

    VMo - Max operating Speed        420 kts IAS
    MMo - Max operating Mach         .85 Mach
    VLe - Max gear operating speed   185 kts IAS
    VMc - Minimum control speed      95 kts IAS

    FLAPS
    Approach -  10º                  220 kts IAS
    Full extension -                 160 kts IAS

    TAKE OFF DECISION SPEED
    Dry runway, flaps up.

    V1 - 110 kts-130kts depending on weight

    ROTATION SPEED
    Dry runway, flaps up.

    Vr - 120 kts

    CRUISE CLIMB

    Sea level to 10,000 ft - 250 kts

    LANDING APPROACH SPEED
    Flaps down, gear down

    120 - 140 kts depending on weight and weather conditions.