CESSNA CITATION II PROCEDURES
This model has been created for entertainment purposes only. This simulation can’t substitute the real flight training. For suggested speeds, see the Reference page of the Kneeboard. Note that most actions can also be performed using the mouse.

To... | Press...
Display/hide GPS | SHIFT+2
Display/hide throttle quadrant | SHIFT+3
Display/hide annunciator panel | SHIFT+4
Display/hide compass | SHIFT+5

SAFETY INSPECTION
[ ] Parking Brake | ON
[ ] Throttle Levers | IDLE
[ ] Fuel Flow | OFF (press CTRL+SHIFT+F1)
[ ] Battery Switch | OFF
[ ] Gear Lever | POSITION “DOWN”
[ ] Flap Handle | ZERO
[ ] Spoilers | RETRACTED
[ ] Elevator Trim | SET TO ZERO
[ ] Aileron / Rudder Trim Tabs | SET
BEFORE START
[ ] Safety Inspection | COMPLETED
[ ] Flight Documents | CHECKED
[ ] Passenger & Cargo Doors | CLOSED AND LOCKED
[ ] Battery Switch | ON
[ ] Warning Displays | ON
[ ] Avionics Master Switch | ON
[ ] DC Volt/Loadmeters | CHECKED
[ ] L and R GEN Switches | OFF
[ ] Flight Controls | CHECKED
[ ] Engine Instruments | CHECKED
[ ] Fuel Quantity | CHECKED
[ ] De-ice devices | OFF
[ ] Aircraft Lighting | OFF
[ ] Weather | ATIS / FLIGHT SERVICES
[ ] Altimeters | SET
[ ] Standby Instruments | SET
[ ] Avionics | SET FOR DEPARTURE
Request Clearance |
[ ] Beacon / Strobe Light | ON
[ ] Transponder | STBY
[ ] Trim | AS DESIRED (with Num Lock off press Num Pad 1 or Num Pad 7 as necessary)
[ ] Takeoff Data (V1, VR, V2) | COMPUTED and SPEEDS SET (see the Reference page of the Kneeboard)
[ ] Departure Briefing | COMPLETED
STARTING ENGINES
Press CTRL+E to initiate engine autostart sequence, or:
[ ] Parking Brake | SET (press CTRL + PERIOD key)
[ ] Thrust Levers | IDLE (press F2 or F3 as necessary)
[ ] Engine Area | CLEAR
[ ] Fuel Flow | ON (press CTRL+SHIFT+F4)
Right Engine: | Start Switch | HOLD
| Fuel Flow | CHECK
| N1 as Increasing N2 | CHECK
| Oil Pressure | CHECK
Left Engine: | Start Switch | HOLD
| Fuel Flow | CHECK
| N1 as Increasing N2 | CHECK
| Oil Pressure | CHECK
[ ] Engine Instruments | CHECK NORMAL
[ ] Warning Lights | OFF
[ ] L and R GEN Switches | ON
[ ] De-ice | ON
BEFORE TAXI
[ ] NAV Lights | ON
[ ] Heading indicador / Altimeters | SET
[ ] Standby Instruments | SET
[ ] Radios | SET FOR DEPARTURE
[ ] Avionics | SET FOR DEPARTURE
[ ] Autopilot | SET and OFF
[ ] Flight Director | ON
[ ] VOR 1 / VOR 2 | SELECT
[ ] Spoiler Lever | RETRACTED
[ ] Flaps | SET (press F6 or F7 as necessary)
[ ] Flight Controls | CHECK
[ ] Aircraft Lighting | ON AS REQUIRED
Request Taxi Clearance |
[ ] Brakes | RELEASE (press PERIOD key)
TAXI - BEFORE TAKEOFF
[ ] L and R LDG-TAXI Light Switches | ON
[ ] Taxi to Runway | 20 KTS. MAX.
[ ] Flight Instruments | CHECK
[ ] Engine Instruments | CHECK
[ ] Autothrottle | ARMED (IF AVAILABLE)
[ ] Takeoff Data (V1, VR, V2) | CHECK (see the Reference page of the Kneeboard)
[ ] Nav Equipment | CHECK
[ ] Transponder | ON
[ ] Flaps | SET FOR TAKEOFF (press F6 or F7 as necessary)
[ ] Trim | SET FOR TAKEOFF (with Num Lock off, press Num Pad 1 or Num Pad 7 as necessary)
[ ] De-ice | AS REQUIRED
[ ] Spoiler Lever | RETRACTED
Request Takeoff Clearance |
TAKEOFF
[ ] Brakes | SET
[ ] Throttle Levers | IDLE
[ ] Spoilers | RETRACTED
[ ] Thrust Lever | T/O (press F3 until T/O)
[ ] Brakes | RELEASE (press PERIOD key)
AFTER TAKEOFF
[ ]After “Positive Rate of Climb” | TOUCH BRAKES SLIGHTLY, THEN GEAR UP
[ ] Flaps | UP AT V2+25
[ ] Yaw Damper | ON AS REQUIRED
[ ] De-ice | AS REQUIRED
[ ] L and R LDG-TAXI Light Switches | OFF
CLIMB
[ ] Autopilot / Autothrottle | CHECK AND SET
[ ] Altimeters | RESET TO 29.92 CROSSING 18,000 FEET
DESCENT
[ ] De-ice | AS REQUIRED
[ ] Altimeters | RESET TO LOCAL CROSSING 18,000 FEET
[ ] Weather | ATIS / FLIGHT SERVICES
[ ] Avionics and Radios | SET
[ ] Fuel Quantities and Balance | CHECK
APPROACH
[ ] Landing Data (VREF, VAPP) | COMPUTED and SPEEDS SET (see the Reference page of the Kneeboard)
[ ] Avionics and Radios | SET
[ ] Flaps | SET (press F6 or F7 as necessary)
[ ] Spoiler Lever | ARM (press SHIFT + / [FORWARD SLASH key])
BEFORE LANDING
[ ] Gear | DN (Check for 3 green lights) (press G)
[ ] L and R LDG-TAXI Light Switches | ON
[ ] Flaps | DN, check indication (press F7 until Dn)
LANDING
[ ] Brakes | AS REQUIRED (press PERIOD key)
[ ] Spoilers | VERIFY EXTENDED
[ ] Thrust Reversers | DEPLOYED AT 60 Kts
AFTER LANDING/CLEARING RUNWAY
[ ] Strobe Lights | OFF
[ ] Transponder | STBY
[ ] De-ice | AS REQUIRED
[ ] L and R LDG-TAXI Light Switches | OFF
[ ] Reverser Lights | VERIFY OFF
[ ] Spoiler Lever | RET (press SHIFT + / (FORWARD SLASH key) until retracted)
[ ] Flaps | UP (press F6 until Up)
[ ] Thrust Levers | IDLE
SHUTDOWN
[ ] Parking Brake | SET (press CTRL + PERIOD key)
[ ] De-Ice | OFF
[ ] Pitot Heat | OFF
[ ] Nav Lights | OFF
[ ] Flight Director | OFF
[ ] Engine Start Switches | OFF
[ ] L and R GEN Switches | OFF
[ ] Thrust Levers | IDLE (press F2 until Idle)
[ ] Fuel Flow | OFF (press CTRL+SHIFT+F1)
[ ] Lights | OFF
[ ] Avionics Master Switch | OFF
[ ] BATT Switch | OFF

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator.