CESSNA CITATION II
REFERENCE INFORMATION
This model has been created for entertainment purposes only. This simulation can’t substitute the real flight training. For standard procedures, see the Checklists tab.

OPERATING LIMITATIONS

WEIGHTS
Maximum Takeoff Weight | 15.900 Lbs.
Maximum Landing Weight | 15.200 Lbs.
Maximum Zero Fuel Weight (Standard) | 11.200 Lbs.
Maximum Zero Fuel Weight (Optional) | 12.200 Lbs.

NOTES: - Maximum takeoff and landing weights may be additionally restricted due to altitude, temperature and field length.

- To adjust fuel load, click Fuel and Load on the Aircraft menu.

AIRSPEED
VMO - Maximum Operating Speed Below FL 140 | 262 KIAS
VMO - Maximum Operating Speed Between FL 140 and FL 280 (9.500 Lbs ZFW) | 277 KIAS
VMO - VMO - Maximum Operating Speed Between FL 140 and FL 305 (9.500 Lbs ZFW) | 262 KIAS
MMO - Maximum Operating Speed Mach | .755 Mach
VLO - Maximum Gear Operating Speed | 200 KIAS
VLE - Maximum Landing Gear Extension Speed | 292 KIAS
VMC - Maximum Control Speed (Airborne) | 85 KIAS
VMCo - Maximum Control Speed (Ground) | 86 KIAS
Turbulent Air Penetration | 180 KIAS
Maximum Tire Ground Speed | 165 Knots
Autopilot Operation | 292 KIAS / 0.755 Mach
TAKEOFF AND LANDING
Maximum Takeoff Altitude | 14.000 Feet
Maximum Tailwind Component | 10 Knots
Maximum Runway Water/Siush Accumulation | 0.5 inch
Maximum Ambient Temperature | ISA +39°C
VMC - Maximum Control Speed (Airborne) | 85 KIAS
VMCo - Maximum Control Speed (Ground) | 86 KIAS
Maximum Tire Ground Speed | 165 Knots

NOTES: - Autopilot and yaw damper must be OFF for takeoff and landing.

- Vertical navigation system must be OFF below 500 feet above ground level.

- This data is not suitable for real-world purposes.