FOKKER-100 PROCEDURES

For suggested Takeoff, Climb ,Cruise, Vref and Landing

data see the Reference page of the Kneeboard.

NOTE: Most actions can also be performed using the mouse.

T O | PRESS
Display/hide Main Panel | SHIFT+1
Display/hide Garmin GPS 530 | SHIFT+2
Display/hide FMC | SHIFT+3
Display/hide Navigational MFD | SHIFT+4
Display/hide Radio Stack | SHIFT+5
Display/hide Ground Handling | SHIFT+6
Display/hide Annunciator Panel | SHIFT+7
Display/hide Throttle Panel | SHIFT+8
Display/hide EICAS | SHIFT+9

[BEFORE START] |
[ ] Main Panel | (SHIFT+1)
[ ] Parking Brake | SET
[ ] Battery | ON
[ ] Avionics | ON
[ ] Nav Lights | ON
[ ] Panel Lights (Night Only) | ON
[ ] ATIS/Clearance | OBTAIN
[ ] FMC | INITITALIZE
[ ] Autopilot Panel | HDG ALT SET
[ ] Beacon | ON
[ ] Pushback | (SHIFT +6)
[ENGINE START] |
[ ] Press CTRL+E | Parameters Chk
| Go To [AFTERSTART]
- or - |
[ ] Press "S" (Middle Start Switch) | Parameters Chk
| Go To [AFTERSTART]
- or - |
[ ] #2 Fuel Valve | OPEN
[ ] #2 Engine | START, Parameters Chk
[ ] #2 Generator Check | # 2 Gen OFF Then ON
[ ] #2 Start Switch | OFF
[ ] #1 Fuel Valve | OPEN
[ ] #1 Engine | START, Parameters Chk
[ ] #1 Generator Check | #1 Gen OFF Then ON
[ ] #1 Start Switch | OFF
[AFTER START] |
[ ] De-ice (Engines Only) | AS REQUIRED
[ ] Pitot Heat | AS REQUIRED
[ ] Flight Controls | CHECK
[ ] Avionics (SHIFT+5) | SET
[ ] Instruments | CHECKED
[ ] FMC | REVIEW
[ ] Trim | SET FOR TO (+25)
[ ] V speeds | Consider (See Reference)
[ ] Flaps | CYCLE SET FOR T.O.
[ ] Spoilers | VERIFY RETRACTED
[TAXI] |
[ ] Taxi Light | ON
[ ] Normal Breaks and Steering | CHECKED
[ ] Thrust Reverses (Check Stow) | CHECKED
[ ] Flight Director (FD) | ON
[ ] HDG ALT Mode | ON Verify CDI Swing
[ ] Flight Instruments | Indicate Proper No Flags
[ ] Flaps | SET FOR TAKEOFF
[BEFORE TAKEOFF] |
[ ] Flaps | SET FOR TAKEOFF
[ ] Trims For Takeoff (+25) | VERIFY SET
[CLEARED FOR TAKEOFF] |
[ ] Brakes | RELEASE
[ ] Landing Light | ON
[ ] Strobe Lights | ON
[ ] Transponder (SHIFT+6) | ALT
[ ] Thrust Levers | SET TO 1.6 EPR
[ ] Airspeed 80 KIAS | CALLOUT "80 KNOTS"
[ ] Airspeed V1 | CALLOUT "V1"
[ ] Airspeed VR | CALLOUT "ROTATE"
>>ROTATE TO 15 DEGREES<< |
[ ] Airspeed V2 | CALLOUT "V2"
[ ] Landing Gear | (Positive Rate) GEAR UP
[ ] Airspeed | V2+15 KIAS to 400 AGL
[ ] Autopilot | ON (ABOVE 500 AGL)
[ ] Flaps | RETRACT BEFORE Vfs
[CLIMB] |
[ ] Set Climb Thrust | 1.4 EPR
[ ] NAV/GPS | AS APPROPRIATE
[ ] Landing/Taxi Lights | OFF ABOVE 10,000' MSL
[ ] Altimeter | 29.92 " ABOVE FL180
[CRUISE] |
[ ] Thrust Levers | SEE Cruise Ref
[ ] Calculate Vref | SEE Landing Ref & FMC
[ ] Autopilot | Monitor
[ ] Review Arrival Procedures | COMPLETE
[DESCENT] |
[ ] Review Approach Procedures | COMPLETE
[ ] De-ice | OFF ABOVE 10C
[ ] Altimeter | SET TO LOCAL FL180
[ ] Avionics | SET SHIFT 6
[ ] Airspeed | <250 KIAS @ 10,000'
[ ] Landing Lights | ON BELOW 10,000' MSL
[ ] Approach Procedures | REVIEW
[APPROACH] |
[ ] NAV/GPS | AS APPROPRIATE
[ ] Airspeed | CHECKED
[ ] De-ice | OFF ABOVE 10 C
[ ] Flaps (Review Speeds) | SET
[ ] Autopilot | CHECKED AND SET
[BEFORE LANDING] |
[ ] Landing Gear | DOWN THREE GREEN
[ ] Flaps | SET FOR LANDING
[ ] Landing Lights | SET
[LANDING ROLL] |
[ ] Thrust Levers | REVERSE
[ ] Speedbrake Lever | FULL UP
[ ] Thrust Levers | IDLE AT 60 KIAS
[ ] Brake | AS REQUIRED
[ ] Autopilot | CHECK DISENGAGED
[TAXI IN] |
[ ] Speedbrake Lever | DOWN
[ ] Flaps | RETRACT
[ ] Transponder | STBY
[ ] Trims | SET (+25)
[ ] Landing, Strobes, Recog. Lights | OFF
[ ] Flight Director | OFF
[ ] De-ice | OFF
[ ] Pitot Heat | OFF
[PARKING/SHUTDOWN] |
[ ] Parking Brake | SET
[ ] Fuel Control Switches | CUTOFF
[ ] Lights | AS REQUIRED
[ ] Avionics | OFF
[ ] Battery | OFF
[ ] Generator Switches Off | OFF

NOTE: This aircraft's real-world checklists have been modified for

use with Flight Simulator.

CHECKLIST AND REFERENCE CHARTS

Mark Lang

Jetblast Creations © 2011

jetblst@gmail.com