FOKKER-100 REFERENCE CHARTS

AIRCRAFT LOADING

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

| General Aircraft Weights |
| Maximum Taxi Weight | 98,500 lbs
| Maximum Take Off Weight (MTOW) | 98,000 lbs
| Maximum Landing Weight | 88,000 lbs

AIRCRAFT SPEEDS

NOTE: See "V-speeds" in the Learning Center Glossary.

| General Aircraft Speeds | KIAS/MACH
Vmo | Maximum Operating Speed | 320
Mmo | Maximum Operating Speed Mach | .77
Vlo | Maximum Gear Operating Speed | 200
Vle | Maximum Gear Extended Speed | 200
Vra | Turbulent Air Penetration Speed | 250 / .65
Vfe | 8 | 250
| 25 | 220
| 42 | 180
| Initial Climb Out | 200
| Maximum Cross Wind Component | 35
| Maximum Tail Wind TO & LDG | 10
| Cruise Climb Below 10,000 | 250
| Cruise Climb Above 10,000 | 280
| Standard Cruise | .70
| Cruise Decent Above 10,000 | 280
| Cruise Decent Below 10,000 | 250
| Approach | 190
| Final Approach | 140
V 1 | Takeoff Decision Speed |
| Flaps 0 | 111
| Flaps 8 | 107
| Flaps 15 | 104
V R | Rotation Speed |
| Flaps 0 | 111
| Flaps 8 | 107
| Flaps 15 | 104
V 2 | Minimum Climb Speed |
| Flaps 0 | 119
| Flaps 8 | 113
| Flaps 15 | 110
V REF | Final Approach Speed |
| Flaps 0 | 129
| Flaps 25 | 117
| Flaps 42 | 109

CRUISE POWER (N1) CHART

5000 | MACH | .38
| TAS | 220
| TGT | 596
10000 | MACH | .39
| TAS | 250
| TGT | 578
25000 | MACH | .70
| TAS | 421
| TGT | 619
31000 | MACH | .70
| TAS | 411
| TGT | 581
32000 | MACH | .70
| TAS | 409
| TGT | 576
33000 | MACH | .70
| TAS | 408
| TGT | 579
34000 | MACH | .70
| TAS | 401
| TGT | 534
35000 | MACH | .70
| TAS | 404
| TGT | 524

NOTE: For best results set power with EICAS and TGT.

NOTE: MFD reads in TAS while STBY ASI reads IAS.

NOTE: Data is based on ISA and Gross Weight.

USEFUL CONFIGURATIONS

EVENT | TAS | TGT | N1 | FLAPS | GEAR
Initial Approach | 220 | 597 | 50 | 8 | UP
Final Approach | 140 | 640 | 54 | 42 | DN

CHECKLIST AND REFERENCE CHARTS

Mark Lang

Jetblast Creations © 2011

jetblst@gmail.com