Boeing 737-200

Microsoft Flight Simulator X

Panel: Pablo Contouris

Pre-Start Checklist

- Parking Brake SET
- Throttle IDLE
- Fuel Flow CUTOFF
- BATT Master Switch ON
- Panel Lights ON if required
- Hydraulic Pump Switches ON
- Landing Gear Lever CHECK DOWN
- Flaps UP
- Spoiler RETRACTED
- APU START / CHECK RUN
- APU Gen ON / CHECK VOLTS
- Fuel Quantity CHECK
- Pitot Heat / De-Ice OFF
- Aircraft Lighting OFF
- Flight controls FREE AND CORRECT
- Passenger Signs OFF
- Check Weather (Atis, Flight Services)
- De-Ice TEST/CHECK
- Request Clearance
- Transponder STANDBY
- Beacon / Anti Collision Lights ON

Startup Checklist

- Thrust Levers IDLE
- Engine Area CLEAR
- Engine Start Switches GND / IGN BOTH
- Fuel Pump Switches ON
- Left Engine

- Master Starter Switch ON
- At N2 > 20% Fuel Flow CHECK ON
- N1 increasing as N2 incr. CHECK
- Oil Pressure CHECK
- Generator Switch ON

- Repeat for right Engine
- Fuel Pump Switches OFF
- APU Gen, APU OFF

Before Taxi Checklist

- Nav Lights ON
- Taxi Lights / Runway Turnoff Lights ON
- Heading Indicator/Altimeters SET
- Standby Instruments SET
- Radios and Avionics SET FOR DEPARTURE
- Autopilot ON, SET, don‘t activate
- Autothrottle ON, SET, don‘t activate
- F/D ON
- Autobrake RTO
- Elevator Trim SET for takeoff
- Request Taxi Clearance

Taxi Checklist

- Parking Brake RELEASE
- Taxi to assigned runway SPEED Max. 20 knots
- Brakes/Gyro/Turn Coordinator CHECK during taxi and turns

Before Take-off Checklist

- Parking Brake SET
- Throttle IDLE
- Elevator Trim SET for takeoff
- Flaps 5 deg
- Spoilers RETRACTED
- Flight Instruments CHECK
- Engine Instruments CHECK
- Takeoff Data (V1, VR, V2) CHECK
- Nav Equipment CHECK
- Landing Lights ON
- Taxi Lights OFF
- Strobe Light ON
- Pitot Heat ON
- De-Ice AS REQUIRED
- Transponder ON
- Request Takeoff Clearance

Take-off Checklist

- Smoothly increase thrust to 60% N1 let spool up
- Takeoff Thrust FULL or TO/GA
- Brakes RELEASE
- V1 = 150 KIAS (descision)
- Vr = 155 KIAS (rotate)
- Pitch 10 deg. nose up
- V2 = 160 KIAS (safety speed)
- At Positive Climb Rate Touch Brakes
- Landing Gear RETRACT
- At 1000' AGL RETRACT Flaps to 1 deg
- At 210 KIAS RETRACT flaps up

Climb-out Checklist

- Throttle AS REQUIRED
- Trim for 250 KIAS / 1800 fpm
- Autopilot/Autothrottle CHECK and ACTIVATE
- Autobrake OFF
- Below 10000' max. speed 250 KIAS
- ATC AS REQUIRED
- Fasten Seat Belts OFF
- No Smoking Sign OFF
- Landing Lights OFF
- Above 10000' speed 280 KIAS

Cruise Checklist (above FL 180)

At Transition Altitude (FL180) set Altimeter to 29,92" (1013mb)

o Accelerate to cruise speed FL180 0.67 mach (330 KIAS)

FL240 0.76 mach (335 KIAS)

FL280 0.80 mach (325 KIAS)

FL330 0.81 mach (295 KIAS)

- Engine+Instruments CHECK
- Fuel Quantity CHECK
- Radios TUNED and SET
- Autopilot CHECK and SET
- Lights as required

Descent Checklist

- Atis/Airport Information CHECK
- Altimeter CHECK
- Radios SET
- De-Ice AS REQUIRED
- Descent Speed to FL240 0.75 mach

to FL180 0.65 mach

At Transition Altitude (FL180) reset Altimeter to local

to FL120 280 KIAS

below 10'000ft 250 KIAS

- Fuel Quantities and Balance CHECK
- Flaps / Landing Gear CHECK UP
- Check Weather (ATIS, Flight Services)

Approach Checklist

Localizer Level Flight :

- Fasten Seat Belts ON
- No Smoking Sign ON
- APU START / CHECK RUN
- APU Gen ON / CHECK VOLTS
- Avionics + Radios SET
- Speed: Establish 210 KIAS
- Landing Lights ON
- Auto Spoilers ARM
- Autobrake SET
- Flaps 5-10 degrees
- Speed: Establish 180 KIAS
- Flaps 15-20 degrees
- Speed: Establish 160 KIAS
- Landing Gear DOWN
- Turning toward runway: set flaps 30 degrees or FULL

Final Glideslope Descent :

- Speed Establish 150 KIAS
- Parking Brake VERIFY OFF
- De-Ice AS REQUIRED

Landing Checklist

- Landing Gear CHECK DOWN
- Autopilot and Autothrottle OFF
- Landing Speed 145 KIAS
- After touchdown Apply Reverse Thrust, at

60 kts: Cancel Reverse Thrust

- Spoilers VERIFY EXTENDED
- Brakes AS REQUIRED

Taxi To Ramp

- Strobe Light OFF
- Autobrake OFF
- Flaps UP
- Spoilers RETRACTED
- Taxi Lights ON
- Landing Lights OFF
- Speed Max. 20 knots
- Transponder 1200 / OFF
- Elevator Trim TAKEOFF SETTING

Shutdown Checklist

- Parking Brake SET
- Throttle IDLE
- Passenger Signs OFF
- Pitot Heat / De-Ice OFF
- Taxi Lights OFF
- Nav Lights OFF
- F/D OFF
- Fuel Flow OFF
- Master Starter Switches OFF
- Beacon / Anti Collision Lights OFF
- Hydraulic Pump Switches OFF
- APU Gen, APU OFF
- BATT Master Switch OFF

Securing Aircraft

- Parking Brake Verify SET
- Throttle Verify IDLE
- All Switches Verify OFF