One-Eleven Panel Manual
Panel Manual | VC extras | Checklists | Flying Tips
Main | Centre | Autopilot | Overhead | Radios
Radios
COM & NAV There are two of these gauges, with one setting COM1 & NAV1 and the other setting COM2 & NAV2 frequencies. The direction for the tuned beacons (NAV1 & NAV2) is shown on the RMI indicator on the main panel (when the RMI is selected as 'VOR'), and the distance to the beacon is shown on the DME instruments (if the beacon supports DME). FS radios work in Whole numbers & Fractions. The frequency is split into two either side of the decimal point. Click on either side of the numbers to increase or decrease the value. Left side to decrease, Right side to increase.
| The selected frequencies on the two radio units can be quickly swapped over by clicking the COM & NAV icon buttons.
ADF frequency There are two of these gauges, with one setting ADF1 & the other setting ADF2 frequencies. The direction to the tuned ADF beacons is shown on the RMI (main panel) when the RMI is selected to 'ADF'. The three knobs at the bottom are used to change the numbers - hundreds, units and decimals. Click either side of the knob to adjust the number up or down.
Transponder FS treats the transponder code as four independant numbers. Click each number to change it. They work by increment only.

Top