One-Eleven Checklists
Panel Manual | VC extras | Checklists | Flying Tips
Speeds | Checklists | Limits
Starting Check
Battery | On
APU Generator Control | Trip (APU Gen Off)
APU | Start To start APU:- Switch 'APU CONTROL' to 'ON' Check 'FUEL VALVE' reads 'OPEN' Click 'PUSH TO START' 'START' gulls eye initially reads 'START' After 35%RPM 'START' goes blank, then displays 'RUN' when at full RPM.
APU Generator Control | Reset (APU Gen On)
Voltage, Cycles, Amps | Check
Start Lever (HP cocks) | Shut
L.P. Valves | Open
Transfer Valves/Pumps | On
Booster pumps | On
APU Air delivery | Open
APU Air crossfeed | Open
Air Con Masters | APU
No smoking signs | On
Seatbelt signs | On
Emergency Lights | Armed
Pitot heat | Check & Off
Anti-icing | Off
Hydraulic Quantity | In green
Hydraulic DC pump | Off
Hydraulic Pumps | Eng & Aux all On
Aileron & Rudder trim | Check & centred
Nav Lights | On
Fuel Aboard | Check gauges v Flight plan
Parking brakes | On
Air Isolation Valves | Open
Air Con Masters | Closed
Ram Air Valve | Closed
Pressure Safety Valve | Open
Eng Generator Control | Trip both (Engine Gens Off)
Start clearance | Obtained from ATC
Beacon | On
Engine Top Temp | On
Throttles | Closed
Start engines | Starting 1 2 To start Engines:- Select 'Start Master' to START. Click 'Start/Relight' switch to 'START & MOTOR' Check for both amber ignitor lights & Green shaft rotation light Start lever will move to OPEN automatically on the model
Start Master | Off
Starter switches | Off
Eng Generator Control | Reset (Engine Gens On)
Bus & Gen Fail lights | Check Out
Air Con Masters | APU
Anti ice | As required
Control surfaces | Checked
Clearence for taxi | Obtained from ATC
Taxi Check
Hydraulic pumps | Aux 1 On, Aux 2 Off
Door warning lights | All Out
Parking brakes | Off
Flaps / Slats | Select for takeoff (18 degrees or 8 if runway length permits)
Pressure Safety Valve | Closed
Battery | Check on
Speed brakes | Checked & zero
Trims | Set for takeoff (3 degrees nose up)
Takeoff speeds | Checked & set (Click the Speed Reference Chinagraph for speeds)
Flight instruments | Checked & set
Reverse | Checked lights out
Flaps | Set for takeoff
Thrust Index | Check Index number (Click top of either Thrust Index gauge to auto set)
Before Takeoff Check
Landing lamps | As required
Pitot heater | On
Windshield Heat | High
Anti-icing | As required
Autopilot | Off
Transponder | Check code
Cabin Pressurization | Check (2000 min selected)
Fuel transfer pumps/valves | Off & Closed (draw fuel from wing tanks only)
Start Switches | Both Relight
Water Injection | On if required
Engine Top Temp | On
Takeoff clearence | Obtained from ATC
After Takeoff Check
Gear | Up, lights out
Flaps | Up at 180 kt
Water Injection | Off
APU | Unless flight time is 1 hour or less 'APU CONTROL' switch to 'OFF'
Start Switches | Off
Landing lamps | Up & off
Air Con Masters | Open
APU Air delivery | Closed
APU Air crossfeed | Closed
Altimeters | Set
Windshield Heat | As required
Hydraulic pumps | Aux 1 & 2 Off
Fuel transfer pumps/valves | On & Open when climb established
Top of Descent Check
Altimeters | Check 29.29 in (1013 mbs)
Safety heights | Check for descent
Cabin Pressurization | Check & set
Approach Check
Cabin Pressurization | Check
APU | Start
No smoking signs | On
Seatbelt signs | On
Emergency Lights | Armed
Windshield Heat | High
Fuel transfer pumps/valves | Off & Closed (draw fuel from wing tanks only)
Booster pumps | All On
Crossfeed valve | Closed
Flaps / Slats | 8 deg max IAS 240, 18 deg max IAS 190, 26+ deg max IAS 180
Speed brakes | Zero
Threshold speed (Vat) | Checked & set (Click the Speed Reference Chinagraph for speeds)
Landing Check
APU | Check running
APU Air delivery | Open
APU Air crossfeed | Open
Air Con Masters | APU
Start Switches | Relight
Hydraulic pumps | Aux 1 On
Gear | Selected down
Altimeters | QFE / QNH checked & set
Airfield & Runway | Checked
Gear check | 3 greens, door lights out
Brakes | Check, parking brake off
Flaps | 45 deg
Landing lamps | Down & On
Autopilot | Off & AP Yaw Damper Off
After Landing Check
Start Switches | Off
Anti-icing | Off
Landing lights | Off
Hydraulic pumps | Aux 1 Off
Flaps | Selected up
Speed brakes/Lift dumpers | Zero
Pitot heater | Off
AP master | Off
Tail trim | Zero
Flaps | Check up
Windshield Heat | As required
Shutdown Check
Parking Brakes | On
Windshield Heat | Off
APU | Checked & on
Eng Generator Control | Trip (Engine Gens Off)
Start Levers | Shut
Engines | Off
Seatbelt signs | Off
Fuel boost pumps | Off
LP Valves | Closed
Beacon | Off
Taxi/Landing lights | Off
Nav lights | Off
Parking Brakes | Off when chocks under
APU Generator Control | Trip (APU Gen Off)
APU | 'APU CONTROL' switch to 'OFF'
Battery | Off

Top