One-Eleven Checklists
Panel Manual | VC extras | Checklists | Flying Tips
Speeds | Checklists | Limits
Speed Limits
Airspeed IAS (VMO): | 336 kts
Mach number (MMO): | 0.78
Max IAS for lowering or raising landing gear: | 230 kts
Max IAS with landing gear down: | VMO
Max IAS with flaps 8 deg: 18 deg: 26 deg: 45 deg | 240 kts 190 kts 180 kts 180 kts
Max altitude for flap extension: | 15,000 ft except in emergency
Max crosswind component Takeoff: Landing: | 30 kts 30 kts
Max IAS with landing lights extended: | 202 kts
Max for emergency descent: | MMO/VMO
Turbulence speeds Climb, cruise & descent: | 290 kts to 30,000 ft, Mach 0.7 above this
Max IAS for screen wipers: | 220 kts
Max speed for air brakes: | No limit, but not to be extended with flaps out except in emergency or on touch down.
Altitude Limits
Max operating altitude: | 34,000 ft
Max altitude for flap extension: | 20,000 ft except in emergency
Weights 500 series
Max takeoff: | 47,400 kg (104,500 lb)
Max landing: | 39,000 kg (85,980 lb)
Max fuel: | 11,195 kg (24,680lb)
Max payload: | 11,984 kg (26,420 lb)
Empty: | 24,758 kg (54,582 lb)
Weights 475 series
Max takeoff: | 44,679 kg (98,500 lb)
Max landing: | 39,000 kg (85,980 lb)
Max fuel: | 11,195 kg (24,680lb)
Max payload: | 9,662 kg (21,300 lb)
Empty: | 23,822 kg (52,518 lb)
Weights 400 series
Max takeoff: | 40,143 kg (88,500 lb)
Max landing: | 35,380 kg (78,000 lb)
Max fuel: | 11,158 kg (24,600lb)
Max payload: | 9,072 kg (20,000 lb)
Empty: | 22,589 kg (49,800 lb)
Weights 200 series
Max takeoff: | 35,834 kg (79,000 lb)
Max landing: | 34,019 kg (75,000 lb)
Max fuel: | 11,158 kg (24,600lb)
Max payload: | 7,983 kg (17,600 lb)
Empty: | 21,047 kg (46,400 lb)
Range Limits 500 series
With max payload: | 1,300 nm
Typical: | 1,600 nm
Range figures are in still air, using long range cruise techniques & no fuel reserves Minimum fuel reserves: Fuel remaining can be as low as 77 kg

Top