Reference Data for Stratojet Albatross |
VMO - Max. authorized speed: | 600 KIAS |
MMO - Max. authorized Mach: | 0.92 mach |
VLO - Max. speed for flaps | 250 KIAS |
VLE - Max. speed for gear down | 250 KIAS |
Cruising speed: | mach 0,75 @ 35.000 ft |
Recommended altitude for cruising speed: | 35.000 ft |
Max. altitude: | 45.000ft |
Range: ~ 7.800 km @ cruising speed and altitude |
(for max. range and best fuel economy: The higher you fly, the lower the fuel consumption) |
Take-off speed: ~ 120 KIAS with flaps 10 |
Min. Landing speed: ~ 90 KIAS with flaps 40 |
Recommended Landing speed: ~ 125 KIAS with flaps 30 |
Recommended flap speeds: |  |
200 KIAS - 175 KIAS: Flaps 10 (to reduce the angle of attack only) |
175 KIAS - 140 KIAS: Flaps 20 |
140 KIAS - 110 KIAS: Flaps 30 |
110 KIAS - 90 KIAS: Flaps 40 |
Technical Data: |  |
Length: | 22,6 m |
Height: | 6,4 m (with gear down) |
Wing span: | 22,2 m |
Empty weight: | 20.000 pounds |
Max gross weight: | 37.500 pounds |
Fuel capacity: | 3x 600 gallons |
Engines: | 2x Rolls Royce AE3007 Turbofan |
Power: | 2x 7.500 lbs |