BOEING F-15E STRIKE EAGLE

REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 61,822 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

NOTE:

To control gauge backlighting in the Virtual Cockpit at night, please use the

Landing Light on/off switch.

VMO - Maximum Operating Speed | 1500 KIAS
MMO - Maximum Operating Speed Mach | 2.30 Mach
VLO - Maximum Gear Operating Speed | 280 KIAS
VLE - Maximum Landing Gear Extension Speed | 300 KIAS
Best Glide Speed (both engines inoperative) | 160 KIAS
Maximum Operating Range (in Ferry Config) | 2050 NM

Maximum Flap Placard Speeds

Flaps degrees | KIAS
15 | 350
35 | 250

V1 - Takeoff Decision Speed

dry runway
Standard temperature, sea level pressure altitude

All conditions | 140 KIAS

VR - Rotation Speed

dry runway
Standard temperature, sea level pressure altitude

13,200 lbs | 170 KIAS
20,200 lbs | 180 KIAS

V2 - Minimum Climb Speed dry runway
Standard temperature, sea level pressure altitude

13,200 lbs | 170 KIAS
20,200 lbs | 180 KIAS

VREF - Landing Approach Speed

flaps 35, gear down
Standard temperature, sea level pressure altitude

13,200 lbs | 160 KIAS
20,200 lbs | 165 KIAS

NOTE

: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.