LET L-410 UVP-E PROCEDURES

For suggested speeds, see the Reference page of the Kneeboard. Note that most actions can also be performed using the mouse.

To... | Press...
Display/hide radio | SHIFT+2
Display/hide GPS | SHIFT+3
Display/hide engine controls | SHIFT+4
Display/hide overhead panel | SHIFT+5

PREPARATION
1. | CVR | ON
2. | PRE-FLIGHT | COMPLETED
3. | SHIP PAPERS AND ODS | ON BOARD
4. | FLIGHT PLAN, JEPPESEN | ON BOARD
5. | FUEL COCKS | SHUT
6. | FUEL SHUT-OFF VALVE | SHUT
7. | POWER LEVER | IDLE
8. | PROP. LEVER | FEATHER
9. | LANDING GEAR | DOWN
10. | PARKING BRAKE | SET
11. | DC POWER I. II. | BAT
12. | INVERTER 36 V | ON
13. | RADIO & INTERCOM | ON
14. | NAVIGATION LIGHTS | ON
15. | FIRE EXTINGUISHER | TESTED
16. | ALTIMETERS (QNH) | SET
17. | RADIO ALTIMETER 0 | SET
18. | RADIOS, AVIONICS, GPS | SET FOR DEP.
19. | FLIGHT DATA RECORDER | SET
20. | SEAT BELTS | FASTENED
21. | FLIGHT CONTROLS | FREE
22. | CARGO PAPERS | ON BOARD
23. | FUEL QUANTITY | ACC OFP
24. | ATIS / TAKE-OFF DATA | RECEIVED
25. | DOORS AND WINDOWS | CLOSED

BEFORE ENGINE START
1. | START-UP CLEARANCE | RECEIVED
2. | BATTERY I. II. | ON
3. | INVERTER 36 V | ON
4. | ENGINE STARTING L-R | ON
5. | IELU L-R | ON
6. | FUEL PUMPS | ON
7. | ANTI COLLISION LIGHTS | ON
8. | FUEL COCK | OPEN
9. | CABIN HEATING | SHUT
10. | PROPELLER | CLEAR FEATHER NOT ROT

AFTER ENGINE START
1. | SYSTEM SWITCHES / SSOS I. II. | ON
2. | GENERATORS | ON
3. | INVERTERS / STBY HORIZON | ON
4. | AVIONICS / MRK / GMK | ON
5. | ABC / PROP. FEATHERING | ON
6. | SEAT BELT / ICE DETECTOR | ON
7. | AMS / DME / RA | ON
8. | RADAR / TRANSPONDER I. II. | STBY-ON
9. | ANNUNCIATER PANEL | CHECKED
10. | ARTIFICAL / TBI (L; R; STBY) | CHECKED
11. | TRIMS FOR TAKE OFF | SET
12. | SPOILER / ABC / AUTO-FEATHERING | ON
13. | NOSE-WHEEL STEERING | MANUAL
14. | BRAKE-ANTISKID | ON
15. | FLAPS 18O OR 0O | ON
16. | WINDSHIELD HEATING | STAGE 1

TAXI
1. | TAXI LIGHTS | ON
2. | BRAKES, STEERING | CHECKED
3. | ß - RANGE | CHECKED
4. | FLIGHT INSTRUMENTS | CHECKED
5. | ATC BRIEFING | COMPLETED

BEFORE TAKE OFF
1. | PROP DEICING | AS RQ.
2. | CABIN HEATING | SHUT
3. | PITOT HEATING | ON
4. | TRANSPONDER | ON-ALT.
5. | NOSEWHEEL STEERING | PEDAL
6. | RWY HEADING | SET / CHECKED
7. | TAKE-OFF CLEARANCE | RECEIVED
8. | LANDING LIGHTS | ON

AFTER TAKE OFF
1. | LANDING LIGHTS | OFF
2. | LANDING GEAR | UP
3. | FLAPS | UP
4. | CLIMB POWER | SET
5. | SPOILER / ABC | OFF
6. | RADIO ALTIMETER (above 2000 feet) | SET
7. | ALTIMETERS (1013) | SET

CRUISE
1. | SEAT BELT SIGN | OFF
2. | ALTIMETERS (1013) | SET/X-CHECKED
3. | CRUISE POWER | SET
4. | AUTO FEATHERING (above 10.000 ft) | OFF

DESCENT
1. | SEAT BELT SIGN | ON
2. | FUEL-QUANTITY | CHECKED
3. | SPOILER / ABC / AUTOFEATHER | ON
4. | ATIS / LANDING DATA | RECEIVED
5. | APPROACH BRIEFING | COMPLETED

APPROACH
1. | TAXI LIGHTS | ON
2. | ALTIMETERS (QNH) | SET/X-CHECKED
3. | RADIO ALTIMETER | SET
4. | NAV. AIDS | SET FOR APP.

FINAL
1. | LANDING LIGHTS | ON
2. | LANDING GEAR | DOWN
3. | FLAPS | SET FOR LANDING
4. | NOSE-WHEEL STEERING | PEDAL
5. | CABIN HEATING | SHUT
6. | RADAR | STBY
7. | LANDING CLEARANCE | RECEIVED
8. | PROPS | FORWARD

AFTER LANDING
1. | TAXI LIGHTS | ON
2. | FLAPS | UP
3. | TRANSPONDER | STBY
4. | RADAR | OFF
5. | PITOT / WINDSHIELD HEATING | OFF
6. | DEICING | OFF

PARKING
1. | PARKING BRAKE | SET
2. | POWER LEVER | IDLE
3. | PROP LEVER | FEATHER
4. | FUEL COCKS | SHUT
5. | FUEL SHUT-OFF VALVE | SHUT
6. | ALL CIRCUIT BREAKERS | OFF
7. | FLIGHT DATA RECORDER | OFF
8. | BATTERY I-II. | OFF
9. | PARKING BRAKE (when chocks ON) | OFF

NOTE: This aircraft's real-world checklists have been NOT modified for Flight Simulator.

FARNAIR Hungary Ltd.