[Tooltips]
sd_6015_p0_001=FIRE SOUND ALARM: %(V:OFF|ON)%
sd_6015_p0_002=GEAR WARNING: %(V:ENABLED|DISABLED)%
sd_6015_p0_003=GEAR WARNING: %(V:ENABLED|DISABLED)%
sd_6015_p0_004=A-SKID: %(V:OFF|ON)%
sd_6015_p0_005=ADI BCKUP PWR: %(V:AUTO|MAN)%
sd_6015_p0_006=ADI BCKUP PWR: %(V:AUTO|MAN)%
sd_6015_p0_007=APU FUEL VALVE: %(V:CLOSED|OPENED)%
sd_6015_p0_008=WARN LTS: %(V:BRT|DIM)%
sd_6015_p0_009=EMERG EXIT LT: %(V:OFF|ON)%
sd_6015_p0_010=WHT DECK FLOOD LT: %(V:OFF|ON)%
sd_6015_p0_011=RED PNL LT: %(V:OFF|ON)%
sd_6015_p0_012=FUEL IND: %(V:SUM|L TANK|R TANK)%
sd_6015_p1_001=ELEC: %(V:OFF|BATTERY|GROUND PWR)%
sd_6015_p1_002=INV1 36V: %(V:OFF|ON)%
sd_6015_p1_003=INV2 36V: %(V:OFF|ON)%
sd_6015_p1_004=115V BCKUP: %(V:AUTO|MAN)%
sd_6015_p1_005=115V BCKUP: %(V:AUTO|MAN)%
sd_6015_p1_006=INV1 115V: %(V:OFF|ON)%
sd_6015_p1_007=INV2 115V: %(V:OFF|ON)%
sd_6015_p1_008=AIR PRESS DROP EMERG: %(V:OFF|ON)%
sd_6015_p1_009=AIR PRESS DROP EMERG: %(V:OFF|ON)%
sd_6015_p1_010=AIR PRESS CONTROL BCKUP: %(V:OFF|ON)%
sd_6015_p1_011=AIR PRESS CONTROL BCKUP: %(V:OFF|ON)%
sd_6015_p1_012=AIR PRESS SYS MASTER EMERG: %(V:OFF|ON)%
sd_6015_p1_013=AIR PRESS SYS MASTER EMERG: %(V:OFF|OPEN|CLOSE)%
sd_6015_p1_014=AIR PRESS SYS SOUND ALARM: %(V:OFF|ON)%
sd_6015_p1_015=AIR PRESS SYS MASTER: %(V:OFF|OPEN|CLOSE)%
sd_6015_p1_016=AIR COND SYS TEMP CNTRL CABIN: %(V:OFF|WARM|COLD|AUTO)%
sd_6015_p1_017=AIR COND SYS TEMP CNTRL DUCT: %(V:OFF|WARM|COLD|AUTO)%
sd_6015_p1_018=BLEEDAIR EXTRACT VALVE: %(V:OFF|OPEN|CLOSE|AUTO)%
sd_6015_p1_019=BLEEDAIR EXTRACT RATIO: %(V:LOW|HIGH)%
sd_6015_p1_020=DECK COND: %(V:LOW|HIGH)%
sd_6015_p1_021=STAIRS PWR: %(V:OFF|ON)%
sd_6015_p1_022=STAIRS: %(V:RETRACT|EXTEND)%
sd_6015_p1_023=STAIRS: %(V:RETRACT|EXTEND)%
sd_6015_p1_024=NO SMOKING SIGNS: %(V:OFF|ON)%
sd_6015_p1_025=RED SPOT LTS: %(V:OFF|ON)%
sd_6015_p1_026=RED SPOT LTS: %(V:OFF|ON)%
sd_6015_p1_027=GENERATOR1: %(V:OFF|ON)%
sd_6015_p1_028=GENERATOR2: %(V:OFF|ON)%
sd_6015_p1_029=GENERATOR3: %(V:OFF|ON)%
sd_6015_p1_030=HEMISPHERE SWITCH: %(V:|NORTH|SOUTH)%
sd_6015_p1_031=MODE SELECTOR: %(V:|MK|GPK)%
sd_6015_p1_032=TEST
sd_6015_p1_033=COURSE SELECTOR
sd_6015_p1_034=GYROUNIT SWITCH: %(V:|AUXL|MAIN)%
sd_6015_p4_001=EMERG ENG1 CUT
sd_6015_p4_002=EMERG ENG2 CUT
sd_6015_p4_003=EMERG ENG3 CUT
sd_6015_p4_004=X-FEED: %(V:OFF|ON)%
sd_6015_p4_005=L FUEL PUMP: %(V:OFF|ON)%
sd_6015_p4_006=R FUEL PUMP: %(V:OFF|ON)%
sd_6015_p4_007=R FUEL PUMP EMERG: %(V:OFF|OFF|ON|ON)%
sd_6015_p4_008=PRESS INSTR PWR: %(V:OFF|ON)%
sd_6015_p4_009=STAB MAIN CONTR: %(V:ON|ON|OFF)%
sd_6015_p4_010=EMERG GEAR EXT: %(V:OFF|OFF|ON|ON)%
sd_6015_p4_011=GEAR: %(V:NEUTRAL|DOWN RDY|DOWN|UP RDY|UP)%
sd_6015_p4_012=FLAPS MAIN: %(V:OFF|NEUTR|EXT|RETRACT)%
sd_6015_p4_013=FLAPS EMERG EXT: %(V:OFF|OFF|ON)%
sd_6015_p4_014=THR REVERSE: %(V:OFF|RDY|OPEN|CLOSE)%
sd_6015_p4_015=FUEL PUMP LO: %(V:OFF|RIGHT|LEFT)%
sd_6015_p4_016=X-FEED TANKS: %(V:OFF|OFF|ON|ON)%
sd_6015_p4_017=X-FEED PUMPS: %(V:OFF|OFF|ON|ON)%
sd_6015_p4_018=HYD PUMP: %(V:AUTO|AUTO|MAN)%
sd_6015_p4_019=AP PWR: %(V:OFF|ON)%
sd_6015_p4_020=AP PITCH HOLD: %(V:OFF|ON)%
sd_6015_p4_021=AP CMD: %(V:OFF|ON)%
sd_6015_p4_022=AP ALT HLD: %(V:OFF|ON)%
sd_6015_p4_023=TRIM AILER
sd_6015_p4_024=TRIM RUDDER
sd_6015_p5_001=NOISE FLTR: %(V:OFF|ON)%
sd_6015_p5_002=NOISE FLTR: %(V:OFF|ON)%
sd_6015_p5_003=L LIGHT LEFT: %(V:OFF|LAND|TAXI)%
sd_6015_p5_004=L LIGHT RIGHT: %(V:OFF|LAND|TAXI)%
sd_6015_p5_005=L LIGHTS %(V:RETRACT|EXTEND)
sd_6015_p5_006=LIGHTS NAV: %(V:OFF|ON)%
sd_6015_p5_007=LIGHTS BCN: %(V:OFF|ON)%
sd_6015_p5_008=ENG1 FUEL VLV: %(V:OFF|OFF|ON|ON)%
sd_6015_p5_009=ENG2 FUEL VLV: %(V:OFF|OFF|ON|ON)%
sd_6015_p5_010=ENG3 FUEL VLV: %(V:OFF|OFF|ON|ON)%
sd_6015_p5_011=WNDSHLD DEICE L: %(V:OFF|ON)%
sd_6015_p5_012=WNDSHLD DEICE L: %(V:OFF|ON)%
sd_6015_p5_013=WNDSHLD DEICE RATE: %(V:LOW|HIGH)%
sd_6015_p5_014=ADF1 ACTIVE FREQ: %(V:LEFT|RIGHT)%
sd_6015_p5_015=ADF2 ACTIVE FREQ: %(V:LEFT|RIGHT)%
sd_6015_p5_016=ANT L-R
sd_6015_p5_017=ANT L-R
sd_6015_p5_018=RCVR: %(V:CW|AM)%
sd_6015_p5_019=RCVR: %(V:CW|AM)%
sd_6015_p6_001=RAD ALTIMETER PWR: %(V:OFF|ON)%
sd_6015_p6_002=XDPR PWR: %(V:OFF|ON)%
sd_6015_p6_003=HIJACK ALARM: %(V:OFF|ON)%
sd_6015_p6_004=MODE: %(V:ILS|VOR-DME)%
sd_6015_p6_005=PWR: %(V:OFF|ON)%
sd_6015_p6_006=APU STARTER ELEC: %(V:OFF|ON)%
sd_6015_p6_007=APU STARTER MODE: %(V:OFF|START|DUMP FUEL|COLD SPIN)%
sd_6015_p6_008=ENG STARTER ELEC: %(V:OFF|ON)%
sd_6015_p6_009=ENG STARTER MODE: %(V:OFF|COLD SPIN|START|DUMP FUEL)%
sd_6015_p6_010=ENG SELECT: %(V:NONE|2|1|3)%
sd_6015_p6_011=MAYDAY TX: %(V:OFF|RDY|ON)%
sd_6015_p7_001=MODE: %(V:ILS|VOR-DME)%
sd_6015_p7_002=PWR: %(V:OFF|ON)%
sd_6015_p7_003=ENG1 DEICE: %(V:OFF|ON)%
sd_6015_p7_004=ENG2 DEICE: %(V:OFF|ON)%
sd_6015_p7_005=ENG3 DEICE: %(V:OFF|ON)%
sd_6015_p7_006=PRESSURIZATION SYS: %(V:OFF|ON)%
sd_6015_p7_007=PITOT HEAT L: %(V:OFF|ON)%
sd_6015_p7_008=PITOT HEAT R: %(V:OFF|ON)%
sd_6015_p7_009=ENG1 ICE WARN: %(V:OFF|ON)%
sd_6015_p7_010=ENG2 ICE WARN: %(V:OFF|ON)%
sd_6015_p8_001=COM1 BUS: %(V:OFF|ON)%
sd_6015_p8_002=CAPT VSI BUS: %(V:OFF|ON)%
sd_6015_p8_003=CAPT ADI MAIN BUS: %(V:OFF|ON)%
sd_6015_p8_004=FUEL IND BUS: %(V:OFF|ON)%
sd_6015_p8_005=LAMP TEST BUS: %(V:OFF|ON)%
sd_6015_p8_006=ENG1 IND BUS: %(V:OFF|ON)%
sd_6015_p8_007=ENG2 IND BUS: %(V:OFF|ON)%
sd_6015_p8_008=ENG3 IND BUS: %(V:OFF|ON)%
sd_6015_p8_009=CAPT ADI BACKUP BUS: %(V:OFF|ON)%
sd_6015_p8_010=ADF1 BUS: %(V:OFF|ON)%
sd_6015_p8_011=XPDR BUS: %(V:OFF|ON)%
sd_6015_p8_012=ELEC 36V BACKUP BUS: %(V:OFF|ON)%
sd_6015_p8_013=INV1 115V BUS: %(V:OFF|ON)%
sd_6015_p8_014=INV2 115V BUS: %(V:OFF|ON)%
sd_6015_p8_015=AUTO BACKUP 115V BUS: %(V:OFF|ON)%
sd_6015_p8_016=ENG1 FIRE ALARM BUS: %(V:OFF|ON)%
sd_6015_p8_017=ENG2 FIRE ALARM BUS: %(V:OFF|ON)%
sd_6015_p8_018=ENG3 FIRE ALARM BUS: %(V:OFF|ON)%
sd_6015_p8_019=STALL WARN BUS: %(V:OFF|ON)%
sd_6015_p8_020=FUEL PUMP AUTO BACKUP BUS: %(V:OFF|ON)%
sd_6015_p8_021=FUEL X-FEED BUS: %(V:OFF|ON)%
sd_6015_p8_022=ENG1 FUEL VALVE BUS: %(V:OFF|ON)%
sd_6015_p8_023=ENG2 FUEL VALVE BUS: %(V:OFF|ON)%
sd_6015_p8_024=ENG3 FUEL VALVE BUS: %(V:OFF|ON)%
sd_6015_p8_025=FIRE EXT 1 BUS: %(V:OFF|ON)%
sd_6015_p8_026=FIRE EXT 2 BUS: %(V:OFF|ON)%
sd_6015_p8_027=FIRE EXT 3 BUS: %(V:OFF|ON)%
sd_6015_p8_028=AIR STARTER IND BUS: %(V:OFF|ON)%
sd_6015_p8_029=GEAR UP HORN BUS: %(V:OFF|ON)%
sd_6015_p8_030=APU IGNIT BUS: %(V:OFF|ON)%
sd_6015_p8_031=ENG1 IGNIT BUS: %(V:OFF|ON)%
sd_6015_p8_032=ENG2 IGNIT BUS: %(V:OFF|ON)%
sd_6015_p8_033=ENG3 IGNIT BUS: %(V:OFF|ON)%
sd_6015_p8_034=FIRE EXT1 VALVE BUS: %(V:OFF|ON)%
sd_6015_p8_035=FIRE EXT2 VALVE BUS: %(V:OFF|ON)%
sd_6015_p8_036=FIRE EXT3 VALVE BUS: %(V:OFF|ON)%
sd_6015_p9_001=COM2 BUS: %(V:OFF|ON)%
sd_6015_p9_002=GROUND PWR BUS: %(V:OFF|ON)%
sd_6015_p9_003=COPLT ADI BUS: %(V:OFF|ON)%
sd_6015_p9_004=GMK COURSE SYS BUS: %(V:OFF|ON)%
sd_6015_p9_005=HYDRO SYS BUS: %(V:OFF|ON)%
sd_6015_p9_006=AUTOPILOT BUS: %(V:OFF|ON)%
sd_6015_p9_007=GEAR IND BUS: %(V:OFF|ON)%
sd_6015_p9_008=SIGNAL ROCKETS BUS: %(V:OFF|ON)%
sd_6015_p9_009=ILS SYS BUS: %(V:OFF|ON)%
sd_6015_p9_010=ADF2 BUS: %(V:OFF|ON)%
sd_6015_p9_011=INV 115V EMERG SWITCH BUS: %(V:OFF|ON)%
sd_6015_p9_012=STAB EMERG BUS: %(V:OFF|ON)%
sd_6015_p9_013=FLAPS EMERG BUS: %(V:OFF|ON)%
sd_6015_p9_014=GEAR EMERG BUS: %(V:OFF|ON)%
sd_6015_p9_015=ANTI ICE SYS BUS: %(V:OFF|ON)%
sd_6015_p9_016=EXTREME BANK IND BUS: %(V:OFF|ON)%
sd_6015_p9_017=AIR COND SYS BUS: %(V:OFF|ON)%
sd_6015_p9_018=STAIRS SERVO BUS: %(V:OFF|ON)%
sd_6015_p9_019=TURBO COOLER UNIT BUS: %(V:OFF|ON)%
sd_6015_p9_020=NOSE LEG STEER BUS: %(V:OFF|ON)%
sd_6015_p9_021=FUEL X-FEED BUS: %(V:OFF|ON)%
sd_6015_p9_022=ENG1 DE ICE BUS: %(V:OFF|ON)%
sd_6015_p9_023=ENG2 DE ICE BUS: %(V:OFF|ON)%
sd_6015_p9_024=ENG3 DE ICE BUS: %(V:OFF|ON)%
sd_6015_p9_025=BRAKE SYS BUS: %(V:OFF|ON)%
sd_6015_p9_026=DECK HEATER BUS: %(V:OFF|ON)%
sd_6015_p9_027=CABIN HEATER BUS: %(V:OFF|ON)%
sd_6015_p9_028=TAXI LIGHT L BUS: %(V:OFF|ON)%
sd_6015_p9_029=LANDING LIGHT L BUS: %(V:OFF|ON)%
sd_6015_p9_030=TAXI LIGHT R BUS: %(V:OFF|ON)%
sd_6015_p9_031=LANDING LIGHT R BUS: %(V:OFF|ON)%
sd_6015_p9_032=ALER TRIM BUS: %(V:OFF|ON)%
sd_6015_p9_033=RUDDER TRIM BUS: %(V:OFF|ON)%
sd_6015_p9_034=STAB MAIN BUS: %(V:OFF|ON)%
sd_6015_p9_035=FLAPS MAIN BUS: %(V:OFF|ON)%
sd_6015_p9_036=GEAR MAIN BUS: %(V:OFF|ON)%
sd_6015_pa_103=MAN FIRE EXTNG ENG BAY1
sd_6015_pa_104=MAN FIRE EXTNG ENG BAY2
sd_6015_pa_105=MAN FIRE EXTNG ENG BAY3
sd_6015_pa_106=MAN FIRE EXTNG ENG1
sd_6015_pa_107=MAN FIRE EXTNG ENG2
sd_6015_pa_108=MAN FIRE EXTNG ENG3
sd_6015_pa_109=MAN FIRE EXTNG APU
sd_6015_pa_110=LTS TEST
sd_6015_pa_111=LTS TEST
sd_6015_p0_101=LTS TEST
sd_6015_p0_102=DIS FIRE ALARM HORN
sd_6015_p0_103=DIS ALARM HYD PUMP 1 FAIL
sd_6015_p0_104=DIS ALARM HYD PUMP 2 FAIL
sd_6015_p0_107=ZERO FUEL TEST
sd_6015_p0_108=FULL FUEL TEST
sd_6015_p0_109=GFORCE RESET
sd_6015_p1_101=LTS TEST
sd_6015_p2_101=ELEV TRIM MAIN
sd_6015_p2_102=ELEV TRIM EMERGENCY
sd_6015_p2_103=AP DISCONNECT
sd_6015_p2_104=COM RADIO TRANSMIT
sd_6015_p2_105=REMOVE YOKE PANEL
sd_6015_p3_101=ELEV TRIM MAIN
sd_6015_p3_102=ELEV TRIM EMERGENCY
sd_6015_p3_103=AP DISCONNECT
sd_6015_p3_104=COM RADIO TRANSMIT
sd_6015_p3_105=REMOVE YOKE PANEL
sd_6015_p4_101=LTS TEST
sd_6015_p4_102=X-FEED SYS TEST
sd_6015_p4_103=ENG1 MID-AIR START
sd_6015_p4_104=ENG2 MID-AIR START
sd_6015_p4_105=ENG3 MID-AIR START
sd_6015_p4_106=EMERG GEAR RETR
sd_6015_p6_101=2-WAY COMM TEST
sd_6015_p6_102=ID TRANSMIT
sd_6015_p6_103=SYS TEST-1
sd_6015_p6_104=SYS TEST-2
sd_6015_p6_105=SYS TEST-3
sd_6015_p6_106=APU START
sd_6015_p6_107=APU STOP
sd_6015_p6_108=ENG START
sd_6015_p6_109=ENG STOP
sd_6015_p6_110=NAV1 IDENT: %(V:OFF|ON)%
sd_6015_p7_101=NAV2 IDENT: %(V:OFF|ON)%
sd_6015_p7_102=SYS TEST-1
sd_6015_p7_103=SYS TEST-2
sd_6015_p7_104=SYS TEST-3
sd_6015_p7_105=LTS TEST
sd_6015_p0_301=IKU: %(V:ADF1|VOR1|VOR2|ADF2)%
sd_6015_p0_302=IKU: %(V:ADF1|VOR1|VOR2|ADF2)%
sd_6015_p5_301=ADF1: %(V:OFF|R-COMP|ANT|MAN)%
sd_6015_p5_302=ADF2: %(V:OFF|R-COMP|ANT|MAN)%
sd_6015_p5_303=ADF1 L: %(L:sd_6015_p5_410,integer)%
sd_6015_p5_304=ADF2 L: %(L:sd_6015_p5_412,integer)%
sd_6015_p5_305=ADF1 R: %(L:sd_6015_p5_411,integer)%
sd_6015_p5_306=ADF2 R: %(L:sd_6015_p5_413,integer)%
sd_6015_p5_307=ADF1 L: %(L:sd_6015_p5_410,integer)%
sd_6015_p5_308=ADF2 L: %(L:sd_6015_p5_412,integer)%
sd_6015_p5_309=ADF1 R: %(L:sd_6015_p5_411,integer)%
sd_6015_p5_310=ADF2 R: %(L:sd_6015_p5_413,integer)%
sd_6015_p5_311=ADF1 L: %(L:sd_6015_p5_410,integer)%
sd_6015_p5_312=ADF2 L: %(L:sd_6015_p5_412,integer)%
sd_6015_p5_313=ADF1 R: %(L:sd_6015_p5_411,integer)%
sd_6015_p5_314=ADF2 R: %(L:sd_6015_p5_413,integer)%
sd_6015_p5_315=ADF1 L: %(L:sd_6015_p5_410,integer)%
sd_6015_p5_316=ADF2 L: %(L:sd_6015_p5_412,integer)%
sd_6015_p5_317=ADF1 R: %(L:sd_6015_p5_411,integer)%
sd_6015_p5_318=ADF2 R: %(L:sd_6015_p5_413,integer)%
sd_6015_p5_319=ADF1 L: %(L:sd_6015_p5_410,integer)%
sd_6015_p5_320=ADF2 L: %(L:sd_6015_p5_412,integer)%
sd_6015_p5_321=ADF1 R: %(L:sd_6015_p5_411,integer)%
sd_6015_p5_322=ADF2 R: %(L:sd_6015_p5_413,integer)%
sd_6015_p6_301=UNITS: %(V:NM|KM)%
sd_6015_p6_302=LEFT VHF RADIO: %(V:COM1|COM2|OFF|ADF1 IDENT|ADF2 IDENT)%
sd_6015_p7_301=UNITS: %(V:NM|KM)%
sd_6015_p7_302=RIGHT VHF RADIO: %(V:COM1|COM2|OFF|ADF1 IDENT|ADF2 IDENT)%
sd_6015_p4_411=PARKING BRAKE: %(V:OFF| | | | | | | | | | | | | |ON)%
sd_6015_pa_508=Fuel PSI: %(L:sd_6015_pa_508,number)%, Oil PSI: %(L:sd_6015_pa_509,number)%, Oil temp: @(round(%(L:sd_6015_pa_510,number)%,0))@ C, @(round(cels2fahr(%(L:sd_6015_pa_510,number)%),0))@ F
sd_6015_pa_511=Fuel PSI: %(L:sd_6015_pa_511,number)%, Oil PSI: %(L:sd_6015_pa_512,number)%, Oil temp: @(round(%(L:sd_6015_pa_513,number)%,0))@ C, @(round(cels2fahr(%(L:sd_6015_pa_513,number)%),0))@ F
sd_6015_pa_514=Fuel PSI: %(L:sd_6015_pa_514,number)%, Oil PSI: %(L:sd_6015_pa_515,number)%, Oil temp: @(round(%(L:sd_6015_pa_516,number)%,0))@ C, @(round(cels2fahr(%(L:sd_6015_pa_516,number)%),0))@ F
sd_6015_pa_517=N1: %(L:sd_6015_pa_517,integer)%, N2: %(L:sd_6015_pa_518,integer)%
sd_6015_pa_519=N1: %(L:sd_6015_pa_519,integer)%, N2: %(L:sd_6015_pa_520,integer)%
sd_6015_pa_521=N1: %(L:sd_6015_pa_521,integer)%, N2: %(L:sd_6015_pa_522,integer)%
sd_6015_pa_523=Stabilizer pos: %(L:sd_6015_pa_523,number)% degrees
sd_6015_pa_524=Celsius: @(round(%(L:sd_6015_pa_524,number)%,0))@ Fahrenheit: @(round(cels2fahr(%(L:sd_6015_pa_524,number)%),0))@
sd_6015_pa_525=Celsius: @(round(%(L:sd_6015_pa_525,number)%,0))@ Fahrenheit: @(round(cels2fahr(%(L:sd_6015_pa_525,number)%),0))@
sd_6015_pa_526=Celsius: @(round(%(L:sd_6015_pa_526,number)%,0))@ Fahrenheit: @(round(cels2fahr(%(L:sd_6015_pa_526,number)%),0))@
sd_6015_pa_527=Flaps pos: @(round(%(L:sd_6015_pa_527,number)%,0))@ degrees
sd_6015_pa_528=TAS: @(round(%(A:XML_AIRSPEED_TRUE,knots)%,0))@ knots, IAS: @(round(%(A:XML_AIRSPEED_INDICATED,knots)%,0))@ knots
sd_6015_p0_502=Bank: @(abs(%(L:sd_6015_p0_502,number)%)>180?abs(abs(%(L:sd_6015_p0_502,number)%)-360):abs(%(L:sd_6015_p0_502,number)%))@, Pitch: @(neg(%(L:sd_6015_p0_406,number)%))@
sd_6015_p0_505=Bank: @(abs(%(L:sd_6015_p0_505,number)%)>180?abs(abs(%(L:sd_6015_p0_505,number)%)-360):abs(%(L:sd_6015_p0_505,number)%))@, Pitch: @(neg(%(L:sd_6015_p0_407,number)%))@
sd_6015_p0_507=Temperature: %(L:sd_6015_p0_507,number)%
sd_6015_p0_508=Celsius: @(round(%(L:sd_6015_p0_508,number)%,0))@ Fahrenheit: @(round(cels2fahr(%(L:sd_6015_p0_508,fahrenheit)%),0))@
sd_6015_p0_509=Turn: %(L:sd_6015_p0_509,number), Ball: %(L:sd_6015_p0_510,number)%, VS: %(L:sd_6015_pa_530,number)%
sd_6015_p0_513=Current: %(L:sd_6015_p0_513,number)%, Minimum: %(L:sd_6015_p0_511,number)%, Maximum: %(L:sd_6015_p0_512,number)%
sd_6015_p0_514=Left: %(L:sd_6015_p0_514,number)%, Right: %(L:sd_6015_p0_515,number)%
sd_6015_p0_516=Left: %(L:sd_6015_p0_516,number)%, Right: %(L:sd_6015_p0_517,number)%
sd_6015_p0_518=Main: %(L:sd_6015_p0_518,number)%, Auxl: %(L:sd_6015_p0_519,number)%
sd_6015_p0_521=Left: %(L:sd_6015_p0_520,number)%, Right: %(L:sd_6015_p0_521,number)%
sd_6015_p0_522=Course: @(norm(abs(%(L:sd_6015_p0_522,integer)%-360)))@, Heading: @(norm(%(L:sd_6015_pa_531,integer)%))@
sd_6015_p0_525=Left tank: %(C:FUEL_QUANTITY_LEFT,integer)% pounds, Right tank: %(C:FUEL_QUANTITY_RIGHT,integer)% pounds
sd_6015_p0_528=%(L:sd_6015_p0_528,number)%
sd_6015_p0_529=Altitude: %(L:sd_6015_p0_529,number)%, Pressure: %(L:sd_6015_p0_418,integer)% Pa, %(L:sd_6015_p0_419,number)% Hg, %(L:sd_6015_p0_420,integer)% mmHg
sd_6015_p1_502=Bank: @(abs(%(L:sd_6015_p1_502,number)%)>180?abs(abs(%(L:sd_6015_p1_502,number)%)-360):abs(%(L:sd_6015_p1_502,number)%))@, Pitch: @(neg(%(L:sd_6015_p1_406,number)%))@
sd_6015_p1_504=Course: @(norm(abs(%(L:sd_6015_p1_504,integer)%-360)))@, Heading: @(norm(%(L:sd_6015_pa_531,integer)%))@
sd_6015_p1_507=ADF1: %(L:sd_6015_p1_507,number)%, ADF2: %(L:sd_6015_p1_508,number)%
sd_6015_p1_514=Voltage: %(L:sd_6015_p1_514,number)%
sd_6015_p1_515=Voltage: %(L:sd_6015_p1_515,number)%
sd_6015_p1_516=Voltage: %(L:sd_6015_p1_516,number)%
sd_6015_p1_517=Ampers: %(L:sd_6015_p1_517,number)%
sd_6015_p1_518=Ampers: %(L:sd_6015_p1_518,number)%
sd_6015_p1_519=Ampers: %(L:sd_6015_p1_519,number)%
sd_6015_p1_520=Ampers: %(L:sd_6015_p1_520,number)%
sd_6015_p1_601=LATITUDE SELECTOR: @(%(L:sd_6015_pa_533,integer)%>0?norm90(90-abs(%(L:sd_6015_pa_533,integer)%)):norm90(abs(%(L:sd_6015_pa_533,integer)%)))@ degrees
sd_6015_pa_701=ASPD LOW
sd_6015_pa_702=EXIT OPEN
sd_6015_pa_703=WARN GEAR
sd_6015_pa_704=BANK L HIGH
sd_6015_pa_705=ADI FAIL
sd_6015_pa_706=BANK R HIGH
sd_6015_pa_707=MARKER
sd_6015_pa_708=VOR1 TO
sd_6015_pa_709=VOR1 FROM
sd_6015_pa_710=CAB ALT HIGH
sd_6015_pa_711=CAB AIR PRESS HIGH
sd_6015_pa_712=INV 36V FAIL
sd_6015_pa_713=INV 115V FAIL
sd_6015_pa_714=OIL PRESS LOW
sd_6015_pa_715=AIR STARTER ON
sd_6015_pa_716=FUEL LOW L
sd_6015_pa_717=FUEL LOW R
sd_6015_pa_718=ENG1 VIB HIGH
sd_6015_pa_719=ENG2 VIB HIGH
sd_6015_pa_720=ENG3 VIB HIGH
sd_6015_pa_721=STALL
sd_6015_pa_722=OUTER MARKER
sd_6015_pa_723=MIDDLE MARKER
sd_6015_pa_724=INNER MARKER
sd_6015_pa_725=STARTER
sd_6015_pa_726=APU OIL PRESS NORM
sd_6015_pa_727=APU FUEL VALVE OPEN
sd_6015_pa_728=APU ON FIRE
sd_6015_pa_729=APU RPM NORM
sd_6015_pa_730=APU RPM HIGH
sd_6015_pa_731=HYD PUMP ENG1 FAIL
sd_6015_pa_732=HYD PUMP ENG2 FAIL
sd_6015_pa_733=RAD ALTIMETER FAIL
sd_6015_pa_734=FIRE
sd_6015_pa_735=CABIN CREW
sd_6015_pa_736=ENG OVERHEAT
sd_6015_pa_737=ICE ENG L
sd_6015_pa_738=ICE ENG R
sd_6015_pa_739=GEN1 FAIL
sd_6015_pa_740=GEN2 FAIL
sd_6015_pa_741=GEN3 FAIL
sd_6015_pa_801=WARN GEAR
sd_6015_pa_805=WARN FLAPS
sd_6015_pa_901=ENG1 BAY ON FIRE
sd_6015_pa_902=ENG2 BAY ON FIRE
sd_6015_pa_903=ENG3 BAY ON FIRE
sd_6015_pa_904=ENG1 ON FIRE
sd_6015_pa_905=ENG2 ON FIRE
sd_6015_pa_906=ENG3 ON FIRE
sd_6015_pa_907=EXTING1 VALVE OPEN
sd_6015_pa_908=EXTING2 VALVE OPEN
sd_6015_pa_909=EXTING3 VALVE OPEN
sd_6015_pa_910=EXTING1 VALVE OPEN
sd_6015_pa_911=EXTING2 VALVE OPEN
sd_6015_pa_912=EXTING3 VALVE OPEN
sd_6015_pa_913=FIRE SND ALARM OFF
sd_6015_pa_914=STAIRS DWN
sd_6015_pa_915=INV 115V FAIL
sd_6015_pa_916=GROUND ELEC CONNECTED
sd_6015_pa_917=DIF AIR PRESS DROP
sd_6015_pa_918=AIR PRESS BCKUP CNTRL UNIT ON
sd_6015_pa_919=AIR PRESS-COND SYS OFF
sd_6015_pa_920=AIR COND SYS TURBO COOLER ON
sd_6015_pa_923=FIRE EXTING1 RDY
sd_6015_pa_924=FIRE EXTING2 RDY
sd_6015_pa_925=FIRE EXTING3 RDY
sd_6015_pa_926=FIRE EXTING4 RDY
sd_6015_p4_901=THR REVERSE ON
sd_6015_p4_902=THR REVERSE OFF
sd_6015_p4_903=THR REVERSE ON
sd_6015_p4_904=THR REVERSE OFF
sd_6015_p4_905=L FUEL PUMP ON
sd_6015_p4_906=R FUEL PUMP ON
sd_6015_p4_907=F TANKS L-R CONNECTED
sd_6015_p4_908=F PUMPS L-R CONNECTED
sd_6015_p4_909=X-FEED SYS FAIL
sd_6015_p4_910=X-FEED SYS OK
sd_6015_p4_911=CHARGE EMERG BRAKES SYS
sd_6015_p4_912=AILER TRIM NEUTR
sd_6015_p4_913=RUDDER TRIM NEUTR
sd_6015_p4_914=AP RDY
sd_6015_p7_901=ENG1 DEICE
sd_6015_p7_902=ENG2 DEICE
sd_6015_p7_903=ENG3 DEICE
sd_6015_pa_537=TAS: @(round(%(A:XML_AIRSPEED_TRUE,knots)%,0))@ knots, IAS: @(round(%(A:XML_AIRSPEED_INDICATED,knots)%,0))@ knots
sd_6015_pa_404=RUS/INTL system (In 2D Subpanels only)
sd_6015_p4_418=CENTER RUDDER TRIMMER
sd_6015_p4_419=CENTER AILERON TRIMMER
sd_6015_pa_408=Open/Close Window
sd_6015_pa_409=Ground startup
sd_6015_p1_302=27V-meter: %(V:GENERATOR1|GENERATOR2|GENERATOR3|GROUND|BATTERY RIGHT|MAIN BUS|BATTERY LEFT)%
sd_6015_p1_303=36V-meter: %(V:INV R Phase 1-2|INV R Phase 1-3|INV R Phase 2-3|INV ADI RES Phase 1-2|INV ADI RES Phase 1-3|INV ADI RES Phase 2-3|INV L Phase 2-3|INV L Phase 1-3|INV L Phase 1-2|INV DA30 Phase 2-3|INV DA30 Phase 1-3|INV DA30 Phase 1-2)%
sd_6015_p1_304=115V-meter: %(V:INV R|INV L|GROUND)%
sd_6015_p23_401=Switch to Captain Seat
sd_6015_p23_402=Switch to Copilot Seat
sd_6015_p23_403=Switch to Central Pedestal
sd_6015_p23_404=Switch to Overhead
sd_6015_p23_405=Switch to Left Panel
sd_6015_p23_406=Switch to Right Panel
sd_6015_p23_407=Toggle Left AZS Panel
sd_6015_p23_408=Toggle Right AZS Panel
sd_6015_p0_401=Switch to Left Panel
sd_6015_p0_402=Switch to Overhead
sd_6015_p0_403=Switch to Central Pedestal
sd_6015_p0_404=Switch to Copilot Seat
sd_6015_p1_401=Switch to Right Panel
sd_6015_p1_402=Switch to Overhead
sd_6015_p1_403=Switch to Central Pedestal
sd_6015_p1_404=Switch to Captain Seat
sd_6015_p4_401=Switch to Captain Seat
sd_6015_p4_402=Switch to Overhead
sd_6015_p4_403=Switch to Copilot Seat
sd_6015_p5_401=Switch to Captain Seat
sd_6015_p5_402=Switch to Central Pedestal
sd_6015_p5_403=Switch to Copilot Seat
sd_6015_p6_401=Switch to Captain Seat
sd_6015_p7_401=Switch to Copilot Seat
sd_6015_pa_748=BANK L HIGH
sd_6015_pa_749=BANK R HIGH
sd_6015_pa_750=VOR1 TO
sd_6015_pa_751=VOR1 FROM
sd_6015_p1_523=Altitude: %(L:sd_6015_p1_523,number)%, Pressure: %(L:sd_6015_p1_409,integer)% Pa, %(L:sd_6015_p1_410,number)% Hg, %(L:sd_6015_p1_411,integer)% mmHg
sd_6015_p4_025=NAV RCVR: %(V:ILS|VOR)%
sd_6015_p4_026=IND LIGHTS: %(V:BRT|DIM)%
sd_6015_p4_301=NAV SYS MODE: %(V:ILS|KATET|SP-50)%
sd_6015_kl_001=POWER: %(V:OFF|ON)%
sd_6015_kl_002=BRIGHTNESS
sd_6015_kl_003=BRIGHTNESS
sd_6015_kl_004=LEFT CURSOR: %(V:OFF|ON)%
sd_6015_kl_005=RIGHT CURSOR: %(V:OFF|ON)%
sd_6015_kl_006=LEFT OUTER
sd_6015_kl_007=LEFT OUTER
sd_6015_kl_008=LEFT INNER
sd_6015_kl_009=LEFT INNER
sd_6015_kl_010=RIGHT OUTER
sd_6015_kl_011=RIGHT OUTER
sd_6015_kl_012=RIGHT INNER
sd_6015_kl_013=RIGHT INNER
sd_6015_kl_014=PULL SCAN: %(V:OFF|ON)%
sd_6015_kl_015=MESSAGE
sd_6015_kl_016=ALTITUDE
sd_6015_kl_017=DIRECT TO
sd_6015_kl_018=CLEAR
sd_6015_kl_019=ENTER
