Boeing B575 (Private) REFERENCE INFORMATION

For standard procedures, see the Checklists tab.

Total aircraft weight with full fuel
           20,414 lbs.

MTOW - Maximum Takeoff weight
           16,500 lbs

MLW - Maximum Landing weight 
           11.139 lbs

VA - Maneuvering Speed
          240 kts IAS

V1 - Decision Speed
          100 kts IAS

V2 - Minimum Speed for safe Takeoff (incl eng. failure)
          114 kts IAS

Vr - Rotate Speed
          115 - 120 kts IAS

Vapp - Approach Speed
          110 kts IAS

VTT - Target Speed Over Threshold
          100 kts IAS

VLE - Maximum Gear Extended Speed
          260 kts IAS

VLO - Maximum Gear Operation Speed
          260 kts IAS  

VFE - Maximum Flaps Extended Speed
           250 kts IAS

VMO - Maximum Structural Cruising Speed
           455 kts IAS

MMO - Max Mach Speed
           Mach 0.92

VS  - Stalling Speed Flaps Up
          94 kts IAS


VSO - Stalling Speed Flaps Landing
          85 kts IAS

Best Glide Speed
          120 kts IAS

NB Speedbrakes can be safely deployed regardless of airspeed.

Ceiling   49,000 ft

Max Range  (Full fuel FL460 Mach 0.71)
           6000 nm (With IFR Reserve)

Takeoff Roll at MTOW to clear 50 ft
           3,500 ft

Landing Roll over 50 ft obstacle
           2,800 ft





NOTE:  For explanations of speeds used on this tab, see "V-speeds" in the Glossary section of Help.
