DOUGLAS C-117D SUPER DC-3
REFERENCE INFORMATION
For standard procedures, see the Checklist tab, or in the VC click the Clipboard in the left side pocket..

Total Weight fully loaded and fuelled | 26,200 lbs

NOTE: There are two ways of adjusting weight:

(1) On the ground, with Parking Brake SET, call up the Control Panel (Shift-2) and cycle through the options given for Total Fuel and/or Total Payload. Middle-click to select.

(2) Or, on the Aircraft menu, click Fuel and Load.

Limit Speeds in Knots I.A.S.

VNE Never Exceed | 220
VNO Normal Operating | 170
VLO Gear Down | 144
VFE Flaps 1/4 | 121
VFE Flaps 1/4 to Full Down | 115
VY Best Rate-of-Climb (sea level) | 120
V1 Rotation Speed | 97
Propeller Unfeathering | 135

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.