BOMBARDIER LEARJET 45
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 19,907 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 330 KIAS
MMO - Maximum Operating Speed Mach | .81 Mach
VA - Maneuvering Speed 12,500 lbs (sea level) | 150 KIAS
VA - Maneuvering Speed 12,500 lbs (20,000 ft) | 163 KIAS
VA - Maneuvering Speed 12,500 lbs (40,000 ft) | 195 KIAS
VA - Maneuvering Speed 20,200 lbs (sea level) | 198 KIAS
VA - Maneuvering Speed 20,200 lbs (20,000 ft) | 225 KIAS
VA - Maneuvering Speed 20,200 lbs (40,000 ft) | 245 KIAS
VLO - Maximum Gear Operating Speed | 200 KIAS
VLE - Maximum Landing Gear Extension Speed | 260 KIAS
Best Glide Speed (both engines inoperative) | 160 KIAS

Maximum Flap Placard Speeds

Flaps degrees | KIAS
8 | 250
20 | 200
40 | 150

V1 - Takeoff Decision Speed dry runway
Standard temperature, sea level pressure altitude

All conditions | 107 KIAS

VR - Rotation Speed dry runway
Standard temperature, sea level pressure altitude

13,200 lbs | 108 KIAS
20,200 lbs | 118 KIAS

Standard temperature, 5,000' pressure altitude

13,200 lbs | 108 KIAS
20,200 lbs | 119 KIAS

V2 - Minimum Climb Speed dry runway
Standard temperature, sea level pressure altitude

13,200 lbs | 120 KIAS
20,200 lbs | 129 KIAS

Standard temperature, 5,000' pressure altitude

13,200 lbs | 120 KIAS
20,200 lbs | 130 KIAS

VREF - Landing Approach Speed flaps 40, gear down
Standard temperature, sea level pressure altitude

13,200 lbs | 102 KIAS
20,200 lbs | 123 KIAS

Standard temperature, 5,000' pressure altitude

13,200 lbs | 103 KIAS
20,200 lbs | 123 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.