BOEING 737-800
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 174,200 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 340 KIAS
MMO - Maximum Operating Speed Mach | .82 Mach
Turbulent Air Penetration Speed | 280 KIAS/.76 Mach
VLO - Maximum Gear Operating Speed | 320 KIAS/.82 Mach
VLE - Maximum Landing Gear Extension Speed | 270 KIAS/.82 Mach

Maximum Flap Placard Speeds

Flaps degrees | KIAS
0 | 340
1 | 250
2 | 250
5 | 250
10 | 210
15 | 200
25 | 190
30 | 175
40 | 162

V1 - Takeoff Decision Speed dry runway
Standard temperature, sea level pressure altitude

90,000 lbs (flaps 5) | 96 KIAS
180,000 lbs (flaps 5) | 153 KIAS

VR - Rotation Speed dry runway
Standard temperature, sea level pressure altitude

90,000 lbs (flaps 5) | 98 KIAS
180,000 lbs (flaps 5) | 156 KIAS

V2 - Minimum Climb Speed dry runway
Standard temperature, sea level pressure altitude

90,000 lbs (flaps 5) | 111 KIAS
180,000 lbs (flaps 5) | 161 KIAS

VREF - Landing Approach Speed gear down

90,000 lbs (flaps 30) | 116 KIAS
90,000 lbs (flaps 40) | 165 KIAS
180,000 lbs (flaps 30) | 109 KIAS
180,000 (flaps 40) | 157 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.