Checklist for De Havilland Otter NG by Stratojet
Before Starting Engine
[ ] | Exterior Inspection | CHECK
[ ] | Parking Brake | SET
[ ] | Gear | DOWN
[ ] | De-Ice | OFF
[ ] | Aircraft Lighting | OFF
[ ] | Battery/Master Switch | ON
[ ] | Avionics | SET
[ ] | GPS/NAV Switch | SET
[ ] | Transponder | SET
[ ] | Radio | ATIS
[ ] | Altimeter | SET
[ ] | Autopilot | OFF / PRESET
[ ] | Heading Indicator | SET
Starting Engine
[ ] | Doors | CLOSED
[ ] | Strobe Lights | ON
[ ] | Beacon Lights | ON
[ ] | Fuel Quantities | CHECK
[ ] | Throttle | IDLE
[ ] | Prop Pitch | MAX
[ ] | Fuel Condition | HIGH
[ ] | Clearance | CHECK
[ ] | Starter | ON
[ ] | Generator | ON
[ ] | Check Gauges | CHECK
Before Taxiing
[ ] | Flight Controls | CHECK
[ ] | Flaps | UP
[ ] | Elevator Trim | SET TO ZERO
[ ] | Prop De-Ice | ON (IF NEEDED)
[ ] | Structure De-Ice | ON (IF NEEDED)
[ ] | Nav. Lights | ON
[ ] | Taxi Lights | ON
[ ] | Flight Instruments | CHECK
[ ] | Parking Brake | RELEASE
While Taxiing
[ ] | Brakes | CHECK
[ ] | Flight Instruments | CHECK ON TURNS
[ ] | Turbines Gauges | CHECK
Before Start / Take-Off
[ ] | Landing Light | ON (IF NEEDED)
[ ] | Flaps | 10 (OR MORE)
After Start / Take-Off
[ ] | Landing Gear | UP
[ ] | Flaps | 0
[ ] | Taxi Lights | OFF
[ ] | Landing Lights | OFF
[ ] | Trim | ADJUST
Landing
[ ] | Autopilot | OFF
[ ] | Landing Lights | ON
[ ] | Taxi Lights | ON
[ ] | Flaps | 30 (OR MORE)
[ ] | Landing Gear | DOWN (UP ON WATER)
Shutdown and Security
[ ] | Parking Brake | SET
[ ] | Prop De-Ice | OFF
[ ] | Structure De-Ice | OFF
[ ] | Fuel Condition | CUT-OFF
[ ] | Lights | OFF
[ ] | Generator | OFF
[ ] | Avionics | OFF
[ ] | Battery / Master | OFF