Nardi FN-333 Riviera Checklist:

PRE FLIGHT CONTROL CHECK
Before flight verify you have full control authority. Perform while sitting on the ground with the engine off.
Elevator Up 25.0
Elevator Down 20.0
Aileron Up 25.0
Aileron Down 18.0
Rudder 25.0

______________________________________________________
STARTUP
Mixture : 100%
Fuel Pump: ON
Fuel Valve: OPEN
Fuel Selector: BOTH
Magnetos: START
Throttle: 0%

______________________________________________________
TAKEOFF
Elevator Trim Set to 0.0 deg
Flaps AS NEEDED (0.0 or 10.0 deg)
Throttle 100% (or derated if possible)
Brakes RELEASE
V1 50 KIAS
V2 60 KIAS - ROTATE
_______________________________________________________
NORMAL CLIMB
Throttle 70%
Airspeed 110 KIAS

_______________________________________________________
CRUISE (FAST)
Throttle 90%
Airspeed 140 KIAS

CRUISE (BEST RANGE)
Throttle 70%
Airspeed 130 KIAS

_______________________________________________________
LANDING
Airspeed - Pattern 70 KIAS
Flaps DOWN
Gear DOWN
Floats UP
Water Rudder UP
Airspeed - Over the Fence 60 KIAS

_______________________________________________________
WATER LANDING
Airspeed - Pattern 70 KIAS
Flaps DOWN
Gear UP
Floats DOWN
Water Rudder AS DESIRED
Airspeed - Over the Fence 60 KIAS

_______________________________________________________

FEDERAL AVIATION AGENCY

| 7A5 Revision 2 NARDI FN-333 April 18, 1963 |

TYPE CERTIFICATE DATA SHEET NO. 7A5

This data sheet which is a part of type certificate No. 7A5 prescribes conditions and limitations under which the product for which the type certificate was issued meets the airworthiness requirements of the Civil Air Regulations.

Type Certificate Holder | NARDI S. A.
| Milan, Italy

I - Model FN-333, 4 PCAmM (Normal Category), approved December 15, 1958

Engine |  | Continental IO-470-P
Fuel * |  | 91/96 Minimum grade aviation gasoline
Engine limits * |  | For all operations, 2600 r.p.m. (250 hp.)
Propeller and |  | 1. Hartzell HC82X20-5L/L8433-H
propeller limits |  |  | 2 blades, metal, constant speed with reversible pitch
|  |  | Maximum diameter 84 in.
|  |  | Maximum diameter 81 in. (No further reduction permitted)
|  |  | Pitch settings at 30 in. sta.:
|  |  | Low 13°, high 27°30', reversed -14°
|  | 2. Hartzell HCA3X20-5L/L8433-6B
|  |  | 3 blades, metal, constant speed with reversible pitch
|  |  | Maximum diameter 78 in.
|  |  | Maximum diameter 76 in. (No further reduction permitted)
|  |  | Pitch settings at 30 in. sta.:
|  |  | Low 12°30", high 28°30', reversed -14°30'

Airspeed limits |  | *Vne (never exceed) | 206 m.p.h. (178 knots)
|  | *Vno (max. structural cruising) | 162 m.p.h. (140 knots)
|  | #Vp (maneuvering speed) | 146.5 m.p.h. (127 knots)
|  | *Vfe (flaps extended in all positions) | 125 m.p.h. (109 knots)
|  | *Vle (landing gear extended) | 125 m.p.h. (109 knots)
|  | *Vfle (wing floats extended) | 125 m.p.h. (109 knots)
|  | *Vwre (water rudder extended) | 206 m.p.h. (178 knots)

C.G. range |  | *(+110) to (+117)
(landing gear extended) |  |
Empty weight C.G. range |  | None
Datum |  | Nose of aircraft
Leveling means |  | Datum pads on left door frame
Maximum weight |  | *3270 lb.
No. seats |  | 4 (2 at +52.1, 2 at +95.3)
Maximum baggage |  | *300 lb. (+95.3)
Fuel capacity |  | 65.8 U.S. gal. (two wing tanks, 32.9 U.S. gal. ea.) (+107.5)
Oil capacity |  | 3.5 U.S. gal. (+141.6). See NOTE 1 for data on system oil.

Control surface movements |  | Wing flaps |  |  |  | Down 45°
|  | Aileron |  | Up 25° |  | Down 18°
|  | Elevator Tab |  | Up 23° |  | Down 23°
|  | Elevator |  | Up 25° |  | Down 20°
|  | Rudder |  | Right 25° |  | Left 25°
|  | Stabilizer |  | Fixed |  |

Serial Nos. eligible |  | The Registro Aeronautico Italiano (RAI) Certificate of Airworthiness endorsed as noted below under "Certification basis" must be submitted for each individual aircraft for which application for certification is made.
Certification basis |  | CAR 10. Type Certificate No. 7A5 issued December 25, 1958. Date of Application for Type Certificate December 3, 1957. Each aircraft and any replacement parts manufactured in Italy must be clearly identified as imported.
|  | A U.S. airworthiness certificate may be issued on the basis of a Certificate of Airworthiness for Export signed by a representative of the Registro Aeronautico Italiano (RAI) containing the following statement: "The airplane covered by this certificate has been examined and found to comply with U.S. Civil Air Regulations Part 3, dated May 15, 1956, including Amendments 3-1, 3-2, 3-3, 3-4 and 3-5, and conforms to TC 7A5."
Equipment |  | The basic required equipment as prescribed in the applicable airworthiness regulations (see Certification Basis) must be installed in the aircraft for certification. In addition, the following item of equipment is required:
|  | (a) Pre-stall warning indicator, Safe Flight Instrument Corp. 164.S

NOTE 1. | Current weight and balance report including list of equipment in certificated empty weight, and loading instructions, must be provided for each aircraft at the time of original certification. The certificated empty weight and corresponding center of gravity locations must include system oil of 1 lb. at (+141.6).
NOTE 2. | The following placards must be displayed on the instrument panel in full view of the pilot:
(a) |  | "THIS AIRPLANE MUST BE OPERATED AS A NORMAL CATEGORY AIRPLANE IN COMPLIANCE WITH THE OPERATING LIMITATIONS STATED IN THE FORM OF PLACARDS, MARKINGS. NO ACROBATIC MANEUVERS, INCLUDING SPINS, ARE APPROVED."
(b) |  | "WARNING: REVERSING PROPELLER IN FLIGHT PROHIBITED. OPERATE REVERSE LEVER IN LOW PITCH ONLY. MAXIMUM 2400 RPM IN REVERSE PITCH."
(c) |  | In addition to the above placards, the prescribed operating limitations indicated by "*" under Section I above, must be displayed by permanent markings.

NOTE 3. This aircraft is approved for night flying when the prescribed equipment is installed.

.....END.....

_______________________________________________________

View Panel Instructions

View Reference