Nardi FN-333 Panel:

Main Panel Instructions :

_____________________________________________________________________________________________

Virtual Cockpit Extra Features:

_____________________________________________________________________________________________

MFD Instructions:

Display: Shows whatever you choose with the buttons below it. D1: Shows DME 1 distance on the display. D2: Shows DME 2 distance on the display. TAS: Shows couurent TAS (ground speed) on the display. ADF: Shows ADF Frequency on the display. WP: Show\Hide Warning Lights Panel. LP: Show\Hide Levers Panel. AW: Show\Hide ATC Window. GP: Show\Hide GPS Window. H: Increase ADF frequency 100s. D: Increase ADF frequency 10s. w: Increase ADF frequency 1s. ID: Toggle ADF ident (audio panel). SP: Show\Hide Switches Panel. EP: Show\Hide Engine Gauges. KB: Show Hide KneeBoard. MW: Show\Hide Map Window.

_____________________________________________________________________________________________

Gear\Float Status Indicator:

1: Gear Down Green Light 2: Gear Transition\Unsafe Light 3: Floats Down Green Light 4: Floats Transition\Unsafe Light 5: FIELD config light: it lights up when gear is down, floats and water rudder are retracrted. 6: WATER config light: it lights up when floats down, and gear i9s retracted.

_____________________________________________________________________________________________

Gear, Float & Water Rud. Pos. Indicator:

1: Water Rudder position indicator 2: Left Float position indicator 3: Right Float position indicator 4: Left Gear light 5: Nose Gear light 6: Right Gear light

_____________________________________________________________________________________________

Fuel Status Indicator:

1: Left LOW FUEL light 2: Right LOW FUEL light 3: Left Fuel Quantity Digital Display 4: Right Fuel Quantity Digital Display 5: Total fuel quantity indicator lights 6: This switch commutes the left display between MAIN and AUX fuel quantity 7: This switch commutes the right display between MAIN and AUX fuel quantity 8: TEST switch: when it is pressed all the displays mark 88.8 and all the leds light up. Click it again to stop rthe testing.

_____________________________________________________________________________________________

Oil Status Indicator:

1: Oil Psi Lights: Avoid max. red light after takeoff by lowering a little your propeller RPM. 2: Oil Temperature lights. During normal flight conditions they should never reach the max. red. light 3: Displays either Oil Temp. or Psi 4: This switch commutes the display to show Oil Temp. or Psi.

_____________________________________________________________________________________________

Back To Reference

Back To Checklist